import matplotlib.pyplot as plt

import datetime

import time

import serial

import numpy as np

import random

import logging\_100mm

# Import our modules

from row\_navigation import Rover, navigate\_to\_point, TOLERANCE, follow\_path\_precisely, update\_rover\_visualization, visualize\_turn

from row\_navigation import RowNavigator

from farm\_safety import SafetyModule

from sleep\_mode import FailsafeModule, GPSFailsafeReason, DriftSeverity, DriftAction

# Import the health check module from the second file

from rover\_health\_check import RoverHealthCheck, HealthCheckFailure

# Import coordinate converter

from coordinate\_converter import CoordinateConverter

import threading

from ntrip\_client import NTRIPClient

from emlid\_gps\_integration import EmlidGPSReader,update\_rover\_from\_emlid, setup\_emlid\_integration

from gps\_system\_monitor import GPSSystemMonitor

import sys

import logging

import os

# Ensure port is available before starting

global\_serial\_connection = None

# At the top of the file, after imports

direct\_test\_completed = False # Add this flag

def direct\_serial\_test():

"""Test direct serial connection like in test.py and keep it open if successful"""

global global\_serial\_connection, direct\_test\_completed

# Only run the test once

if direct\_test\_completed:

print("Direct serial test already completed, reusing connection")

return global\_serial\_connection is not None

print("\n🔬 Testing direct serial connection to COM12...")

# First ensure port is released

comprehensive\_port\_release('COM12')

try:

# Use EXACTLY the same code as your working test.py

ser = serial.Serial(

port='COM12',

baudrate=115200,

bytesize=serial.EIGHTBITS,

parity=serial.PARITY\_NONE,

stopbits=serial.STOPBITS\_ONE,

timeout=1

)

print("✅ Connected to COM12")

# Try to read some data

print("📡 Reading data...")

data\_received = False

for \_ in range(10):

line = ser.readline().decode('utf-8', errors='ignore').strip()

if line:

print(f"📊 Received: {line}")

data\_received = True

time.sleep(0.1)

if data\_received:

print("✅ Successfully received data from COM12")

# IMPORTANT: Don't close the connection, save it for later use

global\_serial\_connection = ser

direct\_test\_completed = True # Mark test as completed

return True

else:

print("⚠️ Connected but no data received")

ser.close()

direct\_test\_completed = True # Mark test as completed

return False

except Exception as e:

print(f"❌ Direct serial test failed: {e}")

direct\_test\_completed = True # Mark test as completed

return False

logging.basicConfig(level=logging.INFO,

format='%(asctime)s - %(levelname)s - %(message)s')

def global\_error\_handler(type, value, traceback):

print(f"❌ Uncaught error: {value}")

cleanup\_resources()

sys.\_\_excepthook\_\_(type, value, traceback)

sys.excepthook = global\_error\_handler

def ensure\_port\_available(port='COM12'):

"""Ensure the port is available before attempting connection"""

print(f"🧹 Ensuring {port} is available...")

# First try to close any existing connections

try:

import serial

temp\_ser = serial.Serial(port)

temp\_ser.close()

print(f"✅ Closed existing connection to {port}")

except:

pass

# Kill any Python processes that might be using serial ports

try:

import psutil

import os

current\_pid = os.getpid()

killed = False

for proc in psutil.process\_iter(['pid', 'name']):

try:

if proc.pid != current\_pid and proc.name().lower() in ['python.exe', 'pythonw.exe']:

print(f"🔫 Terminating {proc.name()} (PID: {proc.pid})")

proc.kill()

killed = True

except:

pass

if killed:

time.sleep(2) # Wait for processes to terminate

except Exception as e:

print(f"⚠️ Process cleanup warning: {e}")

# Use mode command to reset port

try:

import os

os.system(f"mode {port} BAUD=115200 PARITY=N DATA=8 STOP=1")

print(f"✅ Reset {port} settings")

except:

pass

time.sleep(1) # Give OS time to release

return True

def comprehensive\_port\_release(port='COM12'):

"""Comprehensive approach to release a COM port"""

print(f"🔓 Attempting comprehensive release of {port}...")

# 1. Try to close any existing connections

try:

import serial

temp\_ser = serial.Serial(port)

temp\_ser.close()

print("✅ Closed existing connection")

except:

pass

# 2. Reset port using mode command

try:

import os

os.system(f"mode {port} BAUD=115200 PARITY=N DATA=8 STOP=1")

print("✅ Reset port settings")

except:

pass

# 3. Kill potential blocking processes

try:

import psutil

import os

current\_pid = os.getpid()

for proc in psutil.process\_iter(['pid', 'name']):

try:

if proc.pid != current\_pid and proc.name().lower() in [

'python.exe', 'pythonw.exe', 'reachview.exe',

'putty.exe', 'terraterm.exe'

]:

print(f"🔫 Terminating {proc.name()} (PID: {proc.pid})")

proc.kill()

except:

pass

print("✅ Cleaned up processes")

except:

pass

# 4. Wait for OS to fully release the port

import time

time.sleep(3)

print("✅ Port release complete")

return True

def robust\_emlid\_connection(port='COM12'):

"""More robust Emlid connection method"""

print(f"🔌 Attempting robust connection to {port}...")

# First force release the port

comprehensive\_port\_release(port)

# Try with direct file access first

try:

import serial

import time

# Open with exclusive access and minimal settings

ser = serial.Serial(

port=port,

baudrate=115200,

timeout=1,

write\_timeout=1,

exclusive=True

)

# Test if we can read data

print("📡 Testing data reception...")

time.sleep(1)

if ser.in\_waiting > 0:

data = ser.read(ser.in\_waiting)

print(f"✅ Received {len(data)} bytes")

ser.close()

time.sleep(1)

return True

ser.close()

time.sleep(1)

except Exception as e:

print(f"❌ Connection error: {e}")

return False

# Call this before attempting to connect

def is\_port\_permanently\_blocked(port='COM12'):

"""

Performs comprehensive checks to determine if a port is permanently blocked

and cannot be accessed programmatically.

Returns:

tuple: (blocked, reason)

"""

import serial

import subprocess

import os

print(f"🔍 Checking if {port} is permanently blocked...")

# Check 1: Basic port existence

try:

ports = list(serial.tools.list\_ports.comports())

port\_exists = any(p.device == port for p in ports)

if not port\_exists:

return True, f"{port} does not exist in the system"

except:

pass

# Check 2: Try with different access modes

for mode in ['r', 'r+', 'w', 'w+']:

try:

# Try to open the port as a file (low-level)

with open(f"\\\\.\\{port}", mode) as f:

return False, "Port can be accessed at file level"

except:

pass

# Check 3: Try with different serial settings

for baudrate in [9600, 115200, 57600]:

for timeout in [0.1, 1.0]:

try:

ser = serial.Serial(port, baudrate=baudrate, timeout=timeout)

ser.close()

return False, "Port can be accessed with serial library"

except:

pass

# Check 4: Check if it's a system-reserved port

try:

result = subprocess.run(["powershell", "-Command",

f"Get-WmiObject Win32\_SerialPort | Where-Object {{$\_.DeviceID -eq '{port}'}} | Select-Object Name,PNPDeviceID"],

capture\_output=True, text=True)

if "System" in result.stdout:

return True, f"{port} is reserved by the system"

except:

pass

return True, f"{port} appears to be permanently blocked"

# Add after the imports

def display\_gps\_info(emlid\_data):

"""Display current GPS information"""

print("\n=== GPS Status ===")

print(f"Fix Type: {emlid\_data.get('solution\_status', 'Unknown')}")

print(f"Satellites: {emlid\_data.get('satellites', 0)}")

print(f"HDOP: {emlid\_data.get('hdop', 0.0):.2f}")

print(f"Position: {emlid\_data.get('latitude', 0.0):.8f}°N, "

f"{emlid\_data.get('longitude', 0.0):.8f}°E")

print("================\n")

def display\_gps\_status():

"""Display GPS status every 10 seconds"""

while True:

try:

if rover and hasattr(rover, 'gps\_reader') and rover.gps\_reader:

position = rover.gps\_reader.last\_position

if position:

print("\n=== GPS STATUS SUMMARY ===")

print(f"Fix Type: {position.get('fix\_quality', 'Unknown')}")

print(f"Satellites: {position.get('satellites', 0)}")

print(f"HDOP: {position.get('hdop', 99.9):.1f}")

print(f"Position: {position.get('latitude', 0.0):.6f}, {position.get('longitude', 0.0):.6f}")

print("==========================")

time.sleep(10) # Update every 10 seconds

except Exception as e:

print(f"Status display error: {e}")

time.sleep(10)

# Add after the imports section

rover = None

ntrip\_client = None

failsafe = None

gps\_thread = None

def check\_gps\_status():

"""Check GPS quality and connection status"""

global rover

if not rover or not hasattr(rover, 'gps\_reader'):

return False

position = rover.gps\_reader.last\_position

if not position:

return False

satellites = position.get('satellites', 0)

hdop = position.get('hdop', 99.9)

fix\_type = position.get('solution\_status', 'Unknown')

# Log GPS status

print(f"\nGPS Status:")

print(f"Fix Type: {fix\_type}")

print(f"Satellites: {satellites}")

print(f"HDOP: {hdop:.1f}")

# Check minimum requirements

return (satellites >= 4 and

hdop < 5.0 and

fix\_type in ['GPS', 'DGPS', 'RTK Fixed', 'RTK Float'])

def gps\_reading\_loop():

"""GPS data reading loop for real or simulated data"""

while True:

try:

if hasattr(rover, 'gps\_reader') and rover.gps\_reader: # ADDED CHECK

if rover.gps\_reader.simulate\_gps:

fake = simulate\_emlid\_gps\_reading()

logging\_100mm.update\_rover\_position\_from\_emlid(rover, fake)

display\_gps\_info(fake)

else:

# Real GPS data

if rover.gps\_reader.last\_position:

display\_gps\_info(rover.gps\_reader.last\_position)

time.sleep(1.0)

except Exception as e:

print(f"GPS reading error: {e}")

time.sleep(1.0)

def setup\_ntrip(rover, emlid\_reader):

"""Setup NTRIP connection and corrections"""

try:

NTRIP\_CONFIG = {

'host': 'your.ntrip.server.url',

'port': 2101,

'mountpoint': 'MOUNTPOINT',

'user': 'your\_username',

'password': 'your\_password'

}

ntrip\_client = NTRIPClient(\*\*NTRIP\_CONFIG)

# Test NTRIP connection

if not ntrip\_client.connect():

raise Exception("Failed to connect to NTRIP server")

# Start RTCM corrections thread

def stream\_rtcm():

for rtcm\_data in ntrip\_client.get\_corrections():

if hasattr(rover, 'gps\_reader'):

rover.gps\_reader.send\_rtcm\_data(rtcm\_data)

ntrip\_thread = threading.Thread(target=stream\_rtcm, daemon=True)

ntrip\_thread.start()

return True

except Exception as e:

print(f"NTRIP setup failed: {e}")

return False

def setup\_gps\_with\_optional\_ntrip(rover, use\_ntrip=False):

"""Setup GPS with optional NTRIP - SIMPLIFIED VERSION based on working test script"""

try:

print("\n📡 Setting up Emlid GPS integration...")

# Initialize Emlid reader with minimal configuration

emlid\_reader = EmlidGPSReader(port='COM12', baud\_rate=115200, message\_format='nmea')

emlid\_reader.simulate\_gps = False

# Register callback before connection

update\_rover\_from\_emlid(rover, emlid\_reader)

print("✅ Callback registered for Emlid GPS data")

# Try the simple connection approach first (like your test script)

print("\n🔌 Attempting to connect to Emlid GPS...")

if hasattr(emlid\_reader, 'connect\_with\_simple\_approach'):

connection\_success = emlid\_reader.connect\_with\_simple\_approach()

else:

# Fallback to regular connect if the new method isn't available

connection\_success = emlid\_reader.connect()

if connection\_success:

print(f"✅ Connected to Emlid M2 on COM12")

# Start reading with immediate verification

if emlid\_reader.start\_reading():

rover.gps\_reader = emlid\_reader

print("📡 GPS data reading started")

# Verify data reception

print("🔍 Verifying data reception...")

for \_ in range(3): # Check 3 times

time.sleep(1)

if emlid\_reader.last\_position:

print("✅ Live GPS data confirmed")

return True

print("⚠️ No position data detected yet, but connection is active")

return True

else:

print("❌ Failed to start GPS reading")

else:

print("❌ Connection failed")

# If we get here, connection failed - clean up

try:

if hasattr(emlid\_reader, 'stop\_reading'):

emlid\_reader.stop\_reading()

if hasattr(emlid\_reader, 'disconnect'):

emlid\_reader.disconnect()

except:

pass

# Simulation fallback

print("\n📡 GPS Connection Failed")

print("Options:")

print("1) Continue with GPS simulation")

print("2) Abort")

while True:

try:

choice = input("Select option (1/2): ").strip()

if choice == '1':

print("\n🧪 Initializing GPS simulation...")

emlid\_reader = EmlidGPSReader(port='COM12', message\_format='nmea')

emlid\_reader.simulate\_gps = True

rover.gps\_reader = emlid\_reader

update\_rover\_from\_emlid(rover, emlid\_reader)

def simulation\_thread():

while True:

try:

fake\_data = simulate\_emlid\_gps\_reading()

for callback in emlid\_reader.callbacks:

try:

callback(fake\_data)

except Exception as e:

print(f"Callback error: {e}")

time.sleep(0.1)

except Exception as e:

print(f"Simulation error: {e}")

time.sleep(1)

sim\_thread = threading.Thread(target=simulation\_thread, daemon=True)

sim\_thread.start()

print("✅ GPS simulation active")

return False

elif choice == '2':

print("\n❌ Setup aborted by user")

return False

else:

print("Invalid choice - enter 1 or 2")

except Exception as input\_e:

print(f"Input error: {input\_e}")

except Exception as e:

print(f"\n❌ GPS setup error: {e}")

import traceback

traceback.print\_exc()

return False

debug = False

safety = SafetyModule()

def setup\_gps\_direct\_approach(rover):

"""Setup GPS using the already open serial connection"""

global global\_serial\_connection

print("\n📡 Setting up GPS with direct serial approach...")

# Check if we already have an open connection

if not global\_serial\_connection or not global\_serial\_connection.is\_open:

print("❌ No open serial connection available")

return False

try:

# Create a minimal EmlidGPSReader that just uses our working connection

emlid\_reader = EmlidGPSReader(port='COM12', baud\_rate=115200)

emlid\_reader.serial\_connection = global\_serial\_connection # Use our already open connection

emlid\_reader.simulate\_gps = False

# Register callback

update\_rover\_from\_emlid(rover, emlid\_reader)

# Create a custom reading thread that doesn't use the EmlidGPSReader's methods

def custom\_reading\_thread():

error\_count = 0

max\_errors = 10

while True:

try:

if not global\_serial\_connection:

print("❌ No serial connection available")

time.sleep(1)

continue

if not global\_serial\_connection.is\_open:

print("❌ Serial connection is closed, attempting to reopen")

try:

global\_serial\_connection.open()

print("✅ Reopened serial connection")

except Exception as open\_err:

print(f"❌ Failed to reopen connection: {open\_err}")

time.sleep(1)

continue

# Read NMEA data directly

try:

line = global\_serial\_connection.readline().decode('utf-8', errors='ignore').strip()

if line:

# Print NMEA data every 1 second

current\_time = time.time()

if not hasattr(custom\_reading\_thread, 'last\_print\_time') or current\_time - custom\_reading\_thread.last\_print\_time >= 1.0:

print(f"📡 NMEA: {line}")

custom\_reading\_thread.last\_print\_time = current\_time

# Process NMEA data

if line.startswith(('$GPGGA', '$GNGGA')):

parts = line.split(',')

if len(parts) >= 15 and parts[6] != '0' and parts[2] and parts[4]:

try:

# Parse position data

position = {

'latitude': float(parts[2][:2]) + float(parts[2][2:]) / 60.0,

'longitude': float(parts[4][:3]) + float(parts[4][3:]) / 60.0,

'altitude': float(parts[9]) if parts[9] else 0.0,

'satellites': int(parts[7]) if parts[7] else 0,

'hdop': float(parts[8]) if parts[8] else 99.9,

'fix\_quality': {

'0': 'Invalid',

'1': 'GPS',

'2': 'DGPS',

'4': 'RTK Fixed',

'5': 'RTK Float'

}.get(parts[6], 'Unknown')

}

# Apply direction

if parts[3] == 'S':

position['latitude'] = -position['latitude']

if parts[5] == 'W':

position['longitude'] = -position['longitude']

# Update last position

emlid\_reader.last\_position = position

emlid\_reader.last\_update\_time = time.time()

# Call callbacks

for callback in emlid\_reader.callbacks:

try:

callback(position)

except Exception as cb\_e:

print(f"Callback error: {cb\_e}")

except Exception as parse\_e:

print(f"NMEA parsing error: {parse\_e}")

error\_count = 0 # Reset error count on successful read

except Exception as read\_err:

error\_count += 1

print(f"Read error ({error\_count}/{max\_errors}): {read\_err}")

if error\_count >= max\_errors:

print("Too many read errors, resetting connection")

try:

global\_serial\_connection.close()

time.sleep(1)

global\_serial\_connection.open()

print("Connection reset complete")

except:

pass

error\_count = 0

time.sleep(0.5)

continue

time.sleep(0.1) # 10Hz rate

except Exception as e:

print(f"Reading thread error: {e}")

error\_count += 1

if error\_count >= max\_errors:

print("Too many errors in reading thread, resetting")

error\_count = 0

time.sleep(1.0)

# Start our custom reading thread

reading\_thread = threading.Thread(target=custom\_reading\_thread, daemon=True)

reading\_thread.start()

emlid\_reader.reading\_thread = reading\_thread

# Assign to rover

rover.gps\_reader = emlid\_reader

print("✅ GPS setup complete with direct approach")

return True

except Exception as e:

print(f"❌ Direct GPS setup failed: {e}")

return False

def enhanced\_gps\_status\_monitor():

"""Enhanced GPS status monitor with health checks"""

global rover

last\_health\_report = 0

while True:

try:

if rover and hasattr(rover, 'gps\_reader') and rover.gps\_reader: # ADDED CHECK

current\_time = time.time()

# Get health status

health = rover.gps\_reader.check\_health()

# Print detailed status every 10 seconds

if current\_time - last\_health\_report > 10:

print(f"\n=== GPS Health Report [{datetime.datetime.now().strftime('%H:%M:%S')}] ===")

print(f"Connected: {'✅' if health['connected'] else '❌'}")

print(f"Thread Alive: {'✅' if health['thread\_alive'] else '❌'}")

print(f"Simulation Mode: {'🧪' if health['simulation\_mode'] else '📡'}")

print(f"Last Update: {health['last\_update']:.1f}s ago")

if rover.gps\_reader.last\_position:

pos = rover.gps\_reader.last\_position

print(f"Fix Quality: {pos.get('fix\_quality', 'Unknown')}")

print(f"Satellites: {pos.get('satellites', 0)}")

print(f"HDOP: {pos.get('hdop', 99.9):.2f}")

# Quality indicators

if pos.get('fix\_quality') == 'RTK Fixed':

print("🟢 Excellent RTK Fixed")

elif pos.get('fix\_quality') == 'RTK Float':

print("🟡 Good RTK Float")

elif pos.get('fix\_quality') in ['GPS', 'DGPS']:

print("🔴 Basic GPS Fix")

else:

print("⚫ Poor/No Fix")

print("=" \* 50)

last\_health\_report = current\_time

# Check for problems

if health['last\_update'] > 10: # No data for 10 seconds

print("⚠️ WARNING: No GPS data received for 10+ seconds")

if not health['connected'] and not health['simulation\_mode']:

print("⚠️ WARNING: GPS connection lost, attempting recovery...")

try:

rover.gps\_reader.connect(retries=2, retry\_delay=1)

except:

pass

time.sleep(5) # Update every 5 seconds

except Exception as e:

print(f"GPS monitor error: {e}")

time.sleep(5)

def get\_float(prompt):

"""Get a float value from user with error handling"""

while True:

try:

value = float(input(prompt))

return value

except ValueError:

print("⚠️ Please enter a valid number.")

def random\_position\_in\_farm(min\_x, max\_x, min\_y, max\_y, safety\_margin=2.0):

"""Generate a random position inside the farm with a safety margin from boundaries"""

x = random.uniform(min\_x + safety\_margin, max\_x - safety\_margin)

y = random.uniform(min\_y + safety\_margin, max\_y - safety\_margin)

return x, y

def safe\_remove(element):

if element:

try:

element.remove()

return True

except:

if debug: print(f"Warning: failed to remove {element}")

return False

def process\_emlid\_gps\_data(rover, emlid\_data):

"""

Process GPS data from Emlid receiver and update rover position.

This is a standalone version that doesn't rely on class methods.

Args:

rover: The rover instance

emlid\_data: Dictionary with GPS data from Emlid receiver

Returns:

bool: True if position was updated successfully, False otherwise

"""

if not emlid\_data or 'latitude' not in emlid\_data or 'longitude' not in emlid\_data:

print("⚠️ Invalid or missing Emlid GPS data")

return False

try:

# Get the coordinate converter

converter = None

if hasattr(rover, 'coordinate\_converter'):

converter = rover.coordinate\_converter

elif hasattr(rover, 'gps\_logger') and hasattr(rover.gps\_logger, 'converter'):

converter = rover.gps\_logger.converter

else:

print("⚠️ No coordinate converter found")

return False

# Convert lat/lon to UTM

easting, northing = converter.latlon\_to\_utm\_coord(

emlid\_data['latitude'],

emlid\_data['longitude']

)

if easting is None or northing is None:

print("⚠️ Failed to convert lat/lon to UTM")

return False

# Get the correct UTM offsets

utm\_offset\_x = 0

utm\_offset\_y = 0

if hasattr(rover, 'navigator') and hasattr(rover.navigator, 'utm\_offset\_x'):

utm\_offset\_x = rover.navigator.utm\_offset\_x

utm\_offset\_y = rover.navigator.utm\_offset\_y

# Calculate the local coordinates by removing the offsets

local\_x = easting - utm\_offset\_x

local\_y = northing - utm\_offset\_y

# Update rover position

rover.set\_position(local\_x, local\_y)

# Log the update if a logger is available

if hasattr(rover, 'gps\_logger'):

if hasattr(rover.gps\_logger, 'log\_data\_once'):

rover.gps\_logger.log\_data\_once()

return True

except Exception as e:

print(f"Error processing Emlid GPS data: {e}")

return False

def display\_ntrip\_status(ntrip\_client):

print("\n=== NTRIP Status ===")

print(f"Connected: {ntrip\_client.connected}")

print("===================\n")

def handle\_gps\_error(error\_message):

"""Handle GPS errors without disconnecting"""

print(f"⚠️ GPS Error: {error\_message}")

print("Attempting recovery...")

# Just reset the failsafe timers without disconnecting

if hasattr(rover, 'failsafe'):

rover.failsafe.last\_gps\_update = time.time()

if hasattr(rover.failsafe, 'last\_correction\_update'):

rover.failsafe.last\_correction\_update = time.time()

return True # Indicate successful recovery

def setup\_gps\_simple\_approach(rover):

"""Setup GPS using the exact same approach as test.py"""

print("\n📡 Setting up Emlid GPS with simple approach...")

# First ensure all existing connections are closed

try:

from emlid\_gps\_integration import cleanup\_all\_gps\_connections

cleanup\_all\_gps\_connections()

time.sleep(2) # Give OS time to release port

except Exception as e:

print(f"Cleanup error: {e}")

# Force release the port

force\_release\_com\_port('COM12')

# Check if port is permanently blocked

blocked, reason = is\_port\_permanently\_blocked('COM12')

if blocked:

print(f"❌ COM12 is permanently blocked: {reason}")

print(" Cannot proceed with real GPS connection")

return False

try:

# Create a simple serial connection like in test.py

ser = serial.Serial(

port='COM12',

baudrate=115200,

bytesize=serial.EIGHTBITS,

parity=serial.PARITY\_NONE,

stopbits=serial.STOPBITS\_ONE,

timeout=1

)

print("✅ Connected to COM12")

# Initialize the EmlidGPSReader with this connection

emlid\_reader = EmlidGPSReader(port='COM12', baud\_rate=115200)

emlid\_reader.serial\_connection = ser # Use our working connection

# Register callback

update\_rover\_from\_emlid(rover, emlid\_reader)

# Start reading thread

emlid\_reader.start\_reading()

# Assign to rover

rover.gps\_reader = emlid\_reader

return True

except Exception as e:

print(f"❌ Simple GPS setup failed: {e}")

return False

def run\_simulation():

global rover, ntrip\_client, failsafe, global\_serial\_connection

print("🧹 Initial cleanup of any existing GPS connections...")

try:

from emlid\_gps\_integration import cleanup\_all\_gps\_connections

cleanup\_all\_gps\_connections()

except Exception as e:

print(f"Initial cleanup error: {e}")

direct\_serial\_test()

# Initialize gps\_success variable with a default value

gps\_success = False

# Only run the direct serial test if it hasn't been run yet

if not direct\_test\_completed:

direct\_serial\_test()

def on\_failsafe\_triggered(reason):

print(f"⚠️ Failsafe triggered: {reason.value}")

rover.log\_movement("stop") # Stop the rover for safety

# Update the on\_recovery\_attempt function

def on\_recovery\_attempt(reason):

print(f"🔄 Attempting recovery from {reason.value}")

current\_time = time.time()

try:

if reason == GPSFailsafeReason.GPS\_STALE\_DATA or reason == GPSFailsafeReason.GPS\_DATA\_LOSS:

failsafe.last\_gps\_update = current\_time

# Don't disconnect/reconnect, just reset the timer

print("Resetting GPS data timer without disconnecting")

return True

elif reason == GPSFailsafeReason.GPS\_CORRECTION\_STALE:

failsafe.last\_correction\_update = current\_time

print("Resetting GPS correction timer without disconnecting")

return True

elif reason == GPSFailsafeReason.INTERNET\_CONNECTION\_LOST or reason == GPSFailsafeReason.INTERNET\_CONNECTION\_SLOW:

failsafe.last\_internet\_check = current\_time

return True # Continue without internet

elif reason == GPSFailsafeReason.MODULE\_COMMUNICATION\_FAILURE:

failsafe.last\_module\_comm = current\_time

return True

return True

except Exception as e:

print(f"Recovery attempt failed: {e}")

return False

# Add periodic NTRIP status check

print("🚜 Farm Rover Navigation Simulation 🚜")

print("=====================================")

sys.modules['\_\_main\_\_'].global\_serial\_connection = global\_serial\_connection

# -------------------- HEALTH CHECK SECTION --------------------

print("\n🔍 Running rover health checks before simulation...")

# Create the rover first (needed by the health checker)

rover = Rover()

# Initialize the coordinate converter

coordinate\_converter = CoordinateConverter()

rover.coordinate\_converter = coordinate\_converter

# Initialize health checker with the rover instance

health\_checker = RoverHealthCheck(rover)

try:

# Run all health checks

health\_status = health\_checker.run\_all\_checks(simulation\_mode=True)

# Generate and display health report

health\_report = health\_checker.generate\_health\_report()

print(health\_report)

# Check if all systems passed

if not all(health\_status.values()):

print("\n⚠️ One or more health checks failed. Aborting simulation.")

print(" Please address the issues and try again.")

return

print("\n✅ All health checks passed! Proceeding with simulation.")

except HealthCheckFailure as e:

print(f"\n❌ Critical health check failure: {e}")

print(" Simulation cannot proceed until this issue is resolved.")

return

# -------------------- END HEALTH CHECK SECTION --------------------

plt.rcParams['figure.max\_open\_warning'] = 50

failsafe = FailsafeModule()

safety = SafetyModule(failsafe=failsafe)

failsafe.set\_safety\_module(safety)

# Initialize failsafe first

rover.failsafe = failsafe

failsafe.update\_gps\_status(has\_fix=True, satellites=10, hdop=1.0)

failsafe.update\_internet\_status(connected=True, latency=0.1)

failsafe.update\_module\_communication()

failsafe.set\_callbacks(on\_failsafe\_triggered, on\_recovery\_attempt)

# Now initialize GPS logger

gps\_logger = logging\_100mm.initialize\_gps\_logger(rover)

# Inside run\_simulation function, replace the GPS setup section with:

# Enhanced GPS setup with comprehensive error handling

print("\n📡 Setting up Emlid GPS integration...")

# Initialize gps\_success variable with a default value

gps\_success = False

# Try our direct approach using the already open connection

gps\_success = setup\_gps\_direct\_approach(rover)

status\_thread = threading.Thread(target=display\_gps\_status, daemon=True)

status\_thread.start()

# If that fails, fall back to simulation

if not gps\_success:

print("\n⚠️ GPS setup failed. Switching to simulation mode...")

try:

# Clean up any partial setup

if hasattr(rover, 'gps\_reader') and rover.gps\_reader:

rover.gps\_reader.stop\_reading()

rover.gps\_reader.disconnect()

# Setup simulation

emlid\_reader = EmlidGPSReader(port='COM12', message\_format='nmea')

emlid\_reader.simulate\_gps = True

rover.gps\_reader = emlid\_reader

# Register callback for simulation

update\_rover\_from\_emlid(rover, emlid\_reader)

def gps\_simulation\_loop():

while True:

try:

fake = simulate\_emlid\_gps\_reading()

for callback in emlid\_reader.callbacks:

try:

callback(fake)

except Exception as cb\_e:

print(f"Simulation callback error: {cb\_e}")

time.sleep(0.1) # 10Hz simulation

except Exception as sim\_e:

print(f"Simulation error: {sim\_e}")

time.sleep(1.0)

threading.Thread(target=gps\_simulation\_loop, daemon=True).start()

print("🧪 GPS simulation started successfully")

except Exception as sim\_error:

print(f"❌ Even simulation setup failed: {sim\_error}")

print(" This is a critical error - check your imports and dependencies")

# Create row navigator

navigator = RowNavigator(rover)

rover.navigator = navigator

# Start failsafe monitoring

failsafe.start\_monitoring()

navigator.zigzag\_pattern = True

# Load waypoints from CSV file

csv\_loaded = navigator.load\_rows\_from\_csv(r"F:\GPS\task\_2\_waypoints\waypoints\_100mm.csv")

if not csv\_loaded:

print("❌ Failed to load waypoints from CSV. Simulation cannot proceed without waypoints.")

return

# Calculate farm boundaries based on waypoints with margin

margin = 3.0 # Add margin around waypoints

min\_x = min(point[0] for point in navigator.interpolated\_path) - margin

max\_x = max(point[0] for point in navigator.interpolated\_path) + margin

min\_y = min(point[1] for point in navigator.interpolated\_path) - margin

max\_y = max(point[1] for point in navigator.interpolated\_path) + margin

print(f"📏 Dynamic farm boundaries: X [{min\_x:.2f}, {max\_x:.2f}], Y [{min\_y:.2f}, {max\_y:.2f}]")

# Create vertices for the farm boundary

verts = [(min\_x, min\_y), (max\_x, min\_y), (max\_x, max\_y), (min\_x, max\_y)]

# Generate a random entry point

side = random.randint(0, 3)

if side == 0: # Bottom side

entry\_x = random.uniform(min\_x, max\_x)

entry\_y = min\_y

elif side == 1: # Right side

entry\_x = max\_x

entry\_y = random.uniform(min\_y, max\_y)

elif side == 2: # Top side

entry\_x = random.uniform(min\_x, max\_x)

entry\_y = max\_y

else: # Left side

entry\_x = min\_x

entry\_y = random.uniform(min\_y, max\_y)

entry\_point = (entry\_x, entry\_y)

# Set geofence in rover and safety module

rover.set\_geofence(verts, entry\_point)

safety.set\_geofence(verts)

# Generate random starting position inside the farm

random\_x, random\_y = random\_position\_in\_farm(min\_x, max\_x, min\_y, max\_y)

print(f"🎲 Randomly placing rover inside farm at: ({random\_x:.3f}, {random\_y:.3f})")

# Initialize visualization

plt.ion()

fig, ax = plt.subplots(figsize=(10, 8))

ax.set\_title("Rover Farm Navigation Simulation")

# Draw farm boundary

farm\_polygon = plt.Polygon(np.array(verts), closed=True,

facecolor='lightgreen', edgecolor='darkgreen', alpha=0.3)

ax.add\_patch(farm\_polygon)

# Mark random start position

ax.scatter(random\_x, random\_y, c='green', s=80, label='Start (Inside)')

# Setup rover path visualization

path\_line, = ax.plot([], [], 'b-', alpha=0.5, label='Path')

ax.path\_line = path\_line

ax.legend(loc='upper left')

# Set rover starting position (inside farm)

rover.set\_position(random\_x, random\_y, force=True, add\_to\_history=False)

rover.inside\_fence = True # Force the rover to be considered inside the farm

rover.fence\_locked = True # Lock the rover inside the farm

rover.history.append((rover.x, rover.y))

rover\_patch = update\_rover\_visualization(rover, ax, fig)

print("\n🚜 TASK 1: Determining farm navigation plan with zigzag pattern...\n")

# Ensure zigzag pattern is enabled

navigator.zigzag\_pattern = True

# Use the waypoints previously loaded from CSV

safety.set\_waypoints(navigator.interpolated\_path)

# Determine plot boundaries based on waypoints

if navigator.interpolated\_path:

wp\_min\_x = min(point[0] for point in navigator.interpolated\_path)

wp\_max\_x = max(point[0] for point in navigator.interpolated\_path)

wp\_min\_y = min(point[1] for point in navigator.interpolated\_path)

wp\_max\_y = max(point[1] for point in navigator.interpolated\_path)

# Use the wider range between farm boundaries and waypoints

plot\_min\_x = min(min\_x, wp\_min\_x)

plot\_max\_x = max(max\_x, wp\_max\_x)

plot\_min\_y = min(min\_y, wp\_min\_y)

plot\_max\_y = max(max\_y, wp\_max\_y)

# Add a larger margin

margin = max(plot\_max\_x - plot\_min\_x, plot\_max\_y - plot\_min\_y) \* 0.15

ax.set\_xlim(plot\_min\_x - margin, plot\_max\_x + margin)

ax.set\_ylim(plot\_min\_y - margin, plot\_max\_y + margin)

else:

# Fallback to original farm boundaries

margin = 3

ax.set\_xlim(min\_x - margin, max\_x + margin)

ax.set\_ylim(min\_y - margin, max\_y + margin)

ax.grid(True)

# Visualize zigzag row pattern

x\_coords, y\_coords = zip(\*navigator.interpolated\_path)

ax.plot(x\_coords, y\_coords, 'b-', alpha=0.5, label='Zig-Zag Path')

# Mark start and end points

path\_start = navigator.interpolated\_path[0]

path\_end = navigator.interpolated\_path[-1]

ax.scatter(path\_start[0], path\_start[1], c='orange', s=50, marker='s', label='Path Start')

ax.scatter(path\_end[0], path\_end[1], c='red', s=50, marker='o', label='Path End')

fig.canvas.draw\_idle()

plt.pause(0.5)

# --- TASK 1: Navigate directly to the path start point ---

print("\n🚜 TASK 1: Navigating directly to path start point...\n")

print(f"🎯 Path start point: ({path\_start[0]:.3f}, {path\_start[1]:.3f})")

print(f"📏 Distance to path start: {rover.distance\_to(\*path\_start):.3f}m")

def on\_rover\_wakeup():

print("Rover has woken up! Resuming operations...")

# Do whatever you need when rover wakes up

# Navigate to path start

def navigate\_to\_path\_start(rover, safety, path\_start, ax, fig, rover\_patch):

"""

Navigate rover to the starting point of the path using direct point-to-point moves

with a larger step size and a slightly more generous tolerance to avoid getting stuck.

"""

print("\n🗺️ Navigating directly to starting point...")

reached\_start, rover\_patch = navigate\_to\_point(

rover,

path\_start[0],

path\_start[1],

ax,

fig,

rover\_patch,

step\_size=1.5, # larger increments per move

tolerance=0.8 # accept slightly further from the exact point

)

return reached\_start, rover\_patch

# Use our custom function to navigate to path start

reached\_start, rover\_patch = navigate\_to\_path\_start(rover, safety, path\_start, ax, fig, rover\_patch)

if not reached\_start:

print("\n⚠️ Could not reach path start point after multiple attempts.")

print(" Try adjusting simulation parameters or path positioning.")

return

#Force rover position to exactly match path start

rover.set\_position(path\_start[0], path\_start[1], force=True)

rover\_patch = update\_rover\_visualization(rover, ax, fig, rover\_patch)

# Mark path start reached

ax.scatter(path\_start[0], path\_start[1], c='lime', s=80, marker='\*', label='Start Reached')

ax.legend(loc='upper left')

fig.canvas.draw\_idle()

plt.pause(1)

print("\n✅ TASK 1 COMPLETE: Successfully reached path start point")

print(f" Current position: ({rover.x:.3f}, {rover.y:.3f})")

# --- TASK 2: Align to the path direction ---

print("\n🚜 TASK 2: Aligning rover to path direction...\n")

# Find next waypoint (should be index 1 since we're at index 0)

navigator.current\_waypoint\_index = 0 # Force to start at the beginning of the path

next\_point = navigator.interpolated\_path[1]

desired\_heading = navigator.calculate\_heading((rover.x, rover.y), next\_point)

# Align to the path direction

rover\_patch = visualize\_turn(rover, desired\_heading, ax, fig, rover\_patch)

print(f" Aligned rover to heading: {desired\_heading:.1f}°")

print("\n✅ TASK 2 COMPLETE: Successfully aligned to path direction")

# --- TASK 3: Navigate through the path ---

print("\n🚜 TASK 3: Starting path navigation pattern...\n")

# Start navigation from the beginning of the path

navigator.current\_waypoint\_index = 0

path\_success = navigator.navigate\_path(ax, fig, rover\_patch)

if not path\_success:

print("\n⚠️ Failed to navigate path. Simulation halted.")

return

# Mark completion of path

final\_point = navigator.interpolated\_path[-1]

ax.scatter(final\_point[0], final\_point[1], c='green', s=100, marker='\*', label='Mission Complete')

ax.legend(loc='upper left')

fig.canvas.draw\_idle()

plt.pause(1)

print("\n🎉 TASK 3 COMPLETE: Successfully navigated the path")

print("\n🏁 SIMULATION COMPLETE! 🏁")

print(f" Total commands executed: {rover.command\_count}")

print(f" Final position: ({rover.x:.3f}, {rover.y:.3f})")

# Keep plot open until closed manually

plt.ioff()

plt.show(block=True)

logging\_100mm.stop\_gps\_logger(rover)

failsafe.stop\_monitoring()

cleanup\_resources()

def cleanup\_resources():

"""Enhanced cleanup with better error handling"""

global rover, ntrip\_client, failsafe, gps\_thread, global\_serial\_connection

print("\nCleaning up resources...")

try:

if global\_serial\_connection and global\_serial\_connection.is\_open:

try:

global\_serial\_connection.close()

print("✅ Closed global serial connection")

except Exception as e:

print(f"⚠️ Error closing global serial connection: {e}")

global\_serial\_connection = None

# FIRST: Stop all GPS-related threads and connections

if rover and hasattr(rover, 'gps\_reader') and rover.gps\_reader: # ADDED CHECK

print("Stopping GPS reader...")

try:

rover.gps\_reader.stop\_reading() # Stop reading first

time.sleep(1) # Give it time

rover.gps\_reader.disconnect() # Then disconnect

time.sleep(1) # Give OS time to release port

print("✅ GPS disconnected successfully")

except Exception as e:

print(f"⚠️ GPS cleanup error: {e}")

# Cleanup all GPS connections (using our new function)

try:

from emlid\_gps\_integration import cleanup\_all\_gps\_connections

cleanup\_all\_gps\_connections()

except Exception as e:

print(f"⚠️ Global GPS cleanup error: {e}")

if ntrip\_client:

print("Cleaning up NTRIP...")

try:

ntrip\_client.cleanup()

except Exception as e:

print(f"⚠️ NTRIP cleanup error: {e}")

ntrip\_client = None

if rover:

print("Stopping GPS logger...")

try:

logging\_100mm.stop\_gps\_logger(rover)

except Exception as e:

print(f"⚠️ Logger cleanup error: {e}")

if failsafe:

print("Stopping failsafe monitoring...")

try:

failsafe.stop\_monitoring()

except Exception as e:

print(f"⚠️ Failsafe cleanup error: {e}")

try:

plt.close('all')

except Exception as e:

print(f"⚠️ Plot cleanup error: {e}")

print("✅ Cleanup complete")

except Exception as e:

print(f"❌ Cleanup error: {e}")

def simulate\_emlid\_gps\_reading():

"""

Simulate an Emlid GPS reading for testing purposes.

Returns a dictionary with lat/lon coordinates and RTK status.

"""

# These are example coordinates - in a real implementation,

# you would get these from the Emlid GPS receiver

# Randomly choose a solution status for demonstration

solution\_statuses = ["fixed", "float", "single", "dgps"]

solution\_status = random.choice(solution\_statuses)

# Determine appropriate HDOP based on solution status

if solution\_status == "fixed":

hdop = random.uniform(0.01, 0.2)

elif solution\_status == "float":

hdop = random.uniform(0.2, 0.5)

elif solution\_status == "dgps":

hdop = random.uniform(0.5, 1.0)

else: # single

hdop = random.uniform(1.0, 2.0)

return {

'latitude': 28.6139, # Example latitude

'longitude': 77.2090, # Example longitude

'solution\_status': solution\_status, # RTK solution status from Emlid

'satellites': random.randint(8, 15), # Number of satellites

'hdop': hdop, # Horizontal dilution of precision

'fix\_quality': solution\_status.upper(), # Add fix\_quality

'altitude': random.uniform(200, 300), # Add altitude

'speed': random.uniform(0, 5), # Add speed

'heading': random.uniform(0, 360) # Add heading

}

def gps\_status\_monitor():

"""Monitor GPS status and quality"""

global rover

while True:

try:

if rover and hasattr(rover, 'gps\_reader'):

if rover.gps\_reader.last\_position:

fix\_type = rover.gps\_reader.last\_position.get('solution\_status', 'Unknown')

satellites = rover.gps\_reader.last\_position.get('satellites', 0)

hdop = rover.gps\_reader.last\_position.get('hdop', 0.0)

if fix\_type == 'fixed':

print("🟢 RTK Fixed")

elif fix\_type == 'float':

print("🟡 RTK Float")

else:

print("🔴 No RTK")

print(f"Satellites: {satellites}, HDOP: {hdop:.2f}")

time.sleep(5) # Update every 5 seconds

except Exception as e:

print(f"GPS status monitor error: {e}")

time.sleep(1)

def test\_emlid\_integration():

"""

Test function to verify Emlid GPS integration with the rover system.

"""

print("🧪 Testing Emlid GPS integration...")

# Create rover instance

rover = Rover()

# Initialize coordinate converter

converter = CoordinateConverter()

rover.coordinate\_converter = converter

# Create row navigator (needed for UTM offsets)

navigator = RowNavigator(rover)

rover.navigator = navigator

# Set default UTM offsets for testing

navigator.utm\_offset\_x = 380000.0

navigator.utm\_offset\_y = 2044880.0

# Initialize GPS logger

gps\_logger = logging\_100mm.initialize\_gps\_logger(rover)

# Simulate Emlid GPS reading

emlid\_data = simulate\_emlid\_gps\_reading()

print(f"📡 Simulated Emlid GPS reading: Lat={emlid\_data['latitude']}, Lon={emlid\_data['longitude']}")

# Use the built-in function from the logging\_100mm module

success = logging\_100mm.update\_rover\_position\_from\_emlid(rover, emlid\_data)

# Check the result

if success:

print("✅ Successfully processed Emlid GPS data")

print(f"🚜 Rover position (UTM): X={rover.x:.3f}, Y={rover.y:.3f}")

# Calculate the actual global UTM coordinates

actual\_easting = rover.x + rover.navigator.utm\_offset\_x

actual\_northing = rover.y + rover.navigator.utm\_offset\_y

# Convert back to lat/lon for verification

lat, lon = converter.utm\_to\_latlon\_coord(

actual\_easting, actual\_northing,

zone\_number=45, zone\_letter='N' # Make sure to use the correct zone

)

print(f"🌐 Rover position (Lat/Lon): {lat:.6f}, {lon:.6f}")

# Calculate difference from original coordinates

original\_lat = emlid\_data['latitude']

original\_lon = emlid\_data['longitude']

lat\_diff = abs(lat - original\_lat)

lon\_diff = abs(lon - original\_lon)

print(f"📊 Conversion difference: Lat={lat\_diff:.8f}, Lon={lon\_diff:.8f}")

if lat\_diff < 0.0001 and lon\_diff < 0.0001:

print("✅ Conversion accuracy check passed")

else:

print("❌ Conversion accuracy check failed - differences too large")

else:

print("❌ Failed to process Emlid GPS data")

# Cleanup

logging\_100mm.stop\_gps\_logger(rover)

print("🧪 Test completed")

def force\_release\_com\_port(port='COM12'):

"""Force release a COM port using mode command"""

print(f"\n🔧 Forcing release of {port}...")

try:

# Try closing any existing connections

try:

temp\_ser = serial.Serial(port)

temp\_ser.close()

except:

pass

# Use mode command to reset port

os.system(f"mode {port} BAUD=115200 PARITY=N DATA=8 STOP=1")

time.sleep(2) # Give OS time to release

# Kill any Python processes that might be using serial ports

import psutil

current\_pid = os.getpid()

for proc in psutil.process\_iter(['pid', 'name']):

try:

if proc.pid != current\_pid and proc.name().lower() in ['python.exe', 'pythonw.exe']:

proc.kill()

except:

pass

time.sleep(2) # Wait for processes to terminate

print("✅ Port cleanup complete")

return True

except Exception as e:

print(f"⚠️ Port cleanup warning: {e}")

return False

def test\_com12\_availability():

"""Test if COM12 is available"""

print("🧪 Testing COM12 availability...")

try:

ser = serial.Serial(

port='COM12',

baudrate=115200,

timeout=1,

bytesize=serial.EIGHTBITS,

parity=serial.PARITY\_NONE,

stopbits=serial.STOPBITS\_ONE

)

print("✅ COM12 is available and opened successfully")

ser.close()

except serial.SerialException as e:

print(f"❌ Failed to open COM12: {e}")

if "Access is denied" in str(e):

print(" 🔍 COM12 is likely in use by another application or process.")

print(" Please close other programs (e.g., ReachView, PuTTY) and try again.")

if \_\_name\_\_ == "\_\_main\_\_":

try:

print("🚜 Starting Farm Simulation...")

# Force initial cleanup

try:

from emlid\_gps\_integration import cleanup\_all\_gps\_connections

cleanup\_all\_gps\_connections()

comprehensive\_port\_release('COM12')

time.sleep(2) # Give OS time to release ports

print("✅ Initial cleanup complete")

except Exception as e:

print(f"⚠️ Cleanup warning: {e}")

# First, try direct serial connection like in test.py

real\_gps = direct\_serial\_test()

# Run simulation in simulation mode by default

print("\n" + "=" \* 50)

if not real\_gps:

# Set simulation flag in GPS module

import emlid\_gps\_integration

emlid\_gps\_integration.simulate\_gps = True

print("🧪 Running in simulation mode")

run\_simulation()

except KeyboardInterrupt:

print("\n\n🛑 Simulation terminated by user")

except Exception as e:

print(f"\n❌ Simulation error: {e}")

import traceback

traceback.print\_exc()

finally:

cleanup\_resources()

import random

import serial

import time

import json

import threading

from coordinate\_converter import CoordinateConverter

import os

from serial import SerialException

import logging

import datetime

import serial.tools.list\_ports

import psutil

import subprocess

import sys

\_active\_readers = []

simulate\_gps = False # Set to True if you want to force simulation even if Emlid is connected

class EmlidGPSReader:

"""

Class to handle reading GPS data from an Emlid Reach GNSS receiver.

The Emlid receiver outputs NMEA or JSON data which this class parses

and converts to UTM coordinates for the rover navigation system.

"""

def \_\_init\_\_(self, port='COM12', baud\_rate=115200, message\_format='nmea'):

"""

Initialize the Emlid GPS reader.

Args:

port (str): Serial port where the Emlid receiver is connected

baud\_rate (int): Baud rate for serial communication

message\_format (str): Format of the GPS messages ('json' or 'nmea')

"""

global \_active\_readers

self.\_is\_disconnecting = False # Add this flag

self.port = port

self.baud\_rate = baud\_rate

self.message\_format = message\_format

self.serial\_connection = None

self.reading\_thread = None

self.stop\_thread = threading.Event()

self.converter = CoordinateConverter()

self.last\_position = None

self.last\_update\_time = 0

self.callbacks = []

self.simulate\_gps = False

\_active\_readers.append(self)

def validate\_position(self, position):

if not position:

return False

lat = position.get('latitude', 0)

lon = position.get('longitude', 0)

hdop = position.get('hdop', 99.9)

satellites = position.get('satellites', 0)

return (-90 <= lat <= 90 and

-180 <= lon <= 180 and

hdop < 10.0 and satellites >= 4 # More lenient for initial connection

)

def \_\_del\_\_(self):

"""Safe destructor that won't raise exceptions"""

try:

if not self.\_is\_disconnecting: # Only disconnect if not already doing so

self.stop\_reading()

self.disconnect()

except:

pass # Suppress any errors during cleanup

def \_kill\_processes\_using\_port(self, port):

"""Enhanced process killing that excludes current process"""

print(f"🔍 Checking processes using {port}...")

try:

import psutil

import os

current\_pid = os.getpid() # Get our own process ID

# Get all processes using serial ports

for proc in psutil.process\_iter(['pid', 'name']):

try:

# Skip our own process

if proc.pid == current\_pid:

continue

# Only kill known problematic processes

if proc.name().lower() in ['python.exe', 'pythonw.exe', 'reachview.exe',

'putty.exe', 'terraterm.exe']:

print(f"🔫 Terminating {proc.name()} (PID: {proc.pid})")

proc.kill()

time.sleep(0.5)

except (psutil.NoSuchProcess, psutil.AccessDenied):

continue

time.sleep(1) # Reduced wait time

print("✅ Process cleanup complete")

except Exception as e:

print(f"⚠️ Process cleanup warning: {e}")

# Continue even if cleanup fails

def \_check\_port\_availability(self, port):

"""Enhanced port availability check"""

try:

ports = list(serial.tools.list\_ports.comports())

for p in ports:

if p.device == port:

print(f"✅ Found {port}: {p.description}")

if p.hwid:

print(f" Hardware ID: {p.hwid}")

if p.manufacturer:

print(f" Manufacturer: {p.manufacturer}")

# Additional check for FTDI (common for Emlid)

if 'FTDI' in str(p.hwid) or 'ftdi' in str(p.description).lower():

print(" ✅ Detected FTDI device (likely Emlid compatible)")

return True

print(f"❌ {port} not found in available ports")

available = [p.device for p in ports]

if available:

print(f"Available ports: {', '.join(available)}")

return False

except Exception as e:

print(f"Port check error: {e}")

return False

def \_test\_port\_basic\_access(self, port):

"""Test basic port access without full configuration"""

try:

test\_serial = serial.Serial()

test\_serial.port = port

test\_serial.timeout = 0.1

test\_serial.open()

test\_serial.close()

print(f"✅ Basic port access test passed for {port}")

return True

except Exception as e:

print(f"❌ Basic port access test failed for {port}: {e}")

return False

def \_autodetect\_emlid\_port(self):

"""Improved auto-detection of Emlid GPS port"""

print("Searching for Emlid GPS device...")

ports = list(serial.tools.list\_ports.comports())

# Look for Emlid-specific identifiers

emlid\_keywords = ['emlid', 'reach', 'gnss', 'gps', 'ftdi', 'cp210x']

for port in ports:

description = port.description.lower()

manufacturer = (port.manufacturer or '').lower()

hwid = port.hwid.lower()

for keyword in emlid\_keywords:

if keyword in description or keyword in manufacturer or keyword in hwid:

print(f"Found potential Emlid device on {port.device}")

print(f"Description: {port.description}")

return port.device

# If not found by description, try common ports

possible\_ports = ['COM12', 'COM11', 'COM10', 'COM9', 'COM8', 'COM7']

for port\_name in possible\_ports:

for port in ports:

if port.device == port\_name:

if self.\_test\_port\_basic\_access(port\_name):

print(f"Using common port {port\_name}")

return port\_name

# Return first available port as last resort

available\_ports = [p.device for p in ports]

if available\_ports:

print(f"Available ports: {', '.join(available\_ports)}")

return available\_ports[0]

raise Exception("No serial ports found!")

def connect(self, retries=5, retry\_delay=2):

"""Enhanced connect method with better error handling"""

print(f"🔌 Connecting to Emlid GPS on {self.port}...")

# First disconnect if already connected

self.disconnect()

# Verify port exists

if not os.path.exists(f"//./{self.port}"):

print(f"❌ Port {self.port} does not exist")

return False

# Check hardware info

import subprocess

try:

result = subprocess.run(["wmic", "path", "Win32\_PnPEntity", "where",

"Caption like '%COM%'", "get", "Caption,DeviceID,Manufacturer", "/format:list"],

capture\_output=True, text=True)

if self.port in result.stdout:

print(f"✅ Found {self.port}: {result.stdout.split(self.port)[1].split('DeviceID')[0].strip()}")

except Exception as e:

print(f"⚠️ Could not get hardware info: {e}")

# Try different baud rates

baud\_rates = [115200, 57600, 9600] # Try multiple baud rates

for attempt in range(1, retries + 1):

for baud in baud\_rates:

try:

print(f"🔌 Attempt {attempt}/{retries}: Trying {baud} baud...")

# Open with different settings

self.ser = serial.Serial(

port=self.port,

baudrate=baud,

bytesize=serial.EIGHTBITS,

parity=serial.PARITY\_NONE,

stopbits=serial.STOPBITS\_ONE,

timeout=1,

write\_timeout=1,

xonxoff=False,

rtscts=False,

dsrdtr=False

)

# Test if we can read data

print("📡 Testing data reception...")

if self.ser.in\_waiting or self.ser.read():

print(f"✅ Successfully connected to {self.port} at {baud} baud")

return True

except serial.SerialException as e:

print(f"❌ Serial error at {baud} baud: {e}")

print("⏳ Waiting for port to be released...")

except Exception as e:

print(f"❌ Other error: {e}")

finally:

if hasattr(self, 'ser') and self.ser:

self.ser.close()

print(f"Waiting {retry\_delay} seconds before next attempt...")

time.sleep(retry\_delay)

print(f"❌ Failed to connect to {self.port} after {retries} attempts")

return False

def connect\_with\_simple\_approach(self):

"""

Connect using the exact same approach that works in test.py

"""

print(f"\n🔌 Connecting to Emlid GPS on {self.port} using test.py approach...")

# First disconnect if already connected

self.disconnect()

time.sleep(1) # Short delay

try:

# Use EXACTLY the same parameters as in test.py

self.serial\_connection = serial.Serial(

port=self.port,

baudrate=115200,

bytesize=serial.EIGHTBITS,

parity=serial.PARITY\_NONE,

stopbits=serial.STOPBITS\_ONE,

timeout=1

)

print("✅ Connected to Emlid GPS")

# Test if we can read data

time.sleep(0.5) # Give it a moment to receive data

for \_ in range(3): # Try reading a few times

if self.serial\_connection.in\_waiting > 0:

line = self.serial\_connection.readline().decode('utf-8', errors='ignore').strip()

if line:

print(f"📡 Data received: {line}")

return True

time.sleep(0.1)

print("⚠️ Connected but no data received yet")

return True # Still return True as we connected successfully

except Exception as e:

print(f"❌ Connection error: {e}")

if self.serial\_connection:

try:

self.serial\_connection.close()

except:

pass

self.serial\_connection = None

return False

def send\_rtcm\_data(self, rtcm\_bytes: bytes):

"""Send raw RTCM correction bytes to the Emlid unit."""

if self.serial\_connection and self.serial\_connection.is\_open:

try:

self.serial\_connection.write(rtcm\_bytes)

except Exception as e:

print(f"⚠️ Failed to send RTCM data: {e}")

def disconnect(self):

"""Enhanced disconnect with better cleanup and error handling"""

if self.\_is\_disconnecting: # Prevent recursive calls

return

self.\_is\_disconnecting = True

print("🔌 Disconnecting from GPS...")

try:

# Stop reading thread first

if hasattr(self, 'stop\_thread'):

self.stop\_thread.set()

# Wait for thread to finish with timeout

if hasattr(self, 'reading\_thread') and self.reading\_thread:

if self.reading\_thread.is\_alive():

if threading.current\_thread() != self.reading\_thread:

try:

self.reading\_thread.join(timeout=2.0)

except RuntimeError: # Handle "cannot join current thread"

pass

# Close serial connection

if hasattr(self, 'serial\_connection') and self.serial\_connection:

if self.serial\_connection.is\_open:

try:

self.serial\_connection.reset\_input\_buffer()

self.serial\_connection.reset\_output\_buffer()

except:

pass

try:

self.serial\_connection.close()

print(f"✅ Closed connection to {self.port}")

except:

pass

self.serial\_connection = None

# Reset thread event for next connection

if hasattr(self, 'stop\_thread'):

self.stop\_thread.clear()

except Exception as e:

print(f"⚠️ Disconnect warning: {e}")

finally:

self.\_is\_disconnecting = False

time.sleep(0.5) # Short delay after cleanup

print("🔌 Disconnect complete")

def start\_reading(self):

"""Start a thread to continuously read GPS data with better error handling."""

# Stop any existing reading thread first

self.stop\_reading()

time.sleep(0.5)

if not self.serial\_connection or not self.serial\_connection.is\_open:

print("No active connection. Attempting to connect...")

success = self.connect()

if not success:

print("Failed to establish connection. Cannot start reading.")

return False

self.stop\_thread.clear()

self.reading\_thread = threading.Thread(target=self.\_read\_loop, daemon=True)

self.reading\_thread.start()

print("📡 Started GPS data reading thread")

return True

def stop\_reading(self):

"""Stop the GPS reading thread."""

print("🛑 Stopping GPS reading...")

if hasattr(self, 'stop\_thread'):

self.stop\_thread.set()

if hasattr(self, 'reading\_thread') and self.reading\_thread and self.reading\_thread.is\_alive():

try:

self.reading\_thread.join(timeout=3.0)

print("📡 Stopped GPS data reading thread")

except Exception as e:

print(f"Warning: Thread stop error: {e}")

def register\_callback(self, callback\_func):

"""Register a callback function to be called when new GPS data is received."""

if callback\_func not in self.callbacks:

self.callbacks.append(callback\_func)

def unregister\_callback(self, callback\_func):

"""Remove a callback function from the list."""

if callback\_func in self.callbacks:

self.callbacks.remove(callback\_func)

def \_simulate\_gps\_data(self):

"""Return simulated GPS data for testing."""

solution\_statuses = ["RTK Fixed", "RTK Float", "DGPS", "GPS"]

solution\_status = random.choice(solution\_statuses)

if solution\_status == "RTK Fixed":

hdop = random.uniform(0.5, 1.0)

elif solution\_status == "RTK Float":

hdop = random.uniform(1.0, 2.0)

else:

hdop = random.uniform(2.0, 4.0)

return {

'latitude': 28.6139,

'longitude': 77.2090,

'altitude': 216.0,

'satellites': random.randint(8, 15),

'hdop': hdop,

'fix\_quality': solution\_status

}

def \_read\_loop(self):

"""Read GPS data at high frequency (10Hz) with robust error handling"""

consecutive\_errors = 0

max\_consecutive\_errors = 10

while not self.stop\_thread.is\_set():

try:

if self.simulate\_gps:

position = self.\_simulate\_gps\_data()

time.sleep(0.1)

consecutive\_errors = 0 # Reset error counter

else:

# Check connection health

if not self.serial\_connection or not self.serial\_connection.is\_open:

print("⚠️ Connection lost, attempting to reconnect...")

if not self.connect():

consecutive\_errors += 1

if consecutive\_errors >= max\_consecutive\_errors:

print("❌ Too many connection failures, switching to simulation mode")

self.simulate\_gps = True

continue

time.sleep(1)

continue

consecutive\_errors = 0

# Read data based on format

try:

data = self.\_read\_nmea() if self.message\_format == 'nmea' else self.\_read\_json()

consecutive\_errors = 0 # Reset on successful read

except Exception as read\_error:

print(f"Read error: {read\_error}")

consecutive\_errors += 1

if consecutive\_errors >= max\_consecutive\_errors:

print("❌ Too many read errors, attempting reconnection...")

self.disconnect()

continue

time.sleep(0.1)

continue

if data:

position = data

print(f"\n=== GPS Update [{datetime.datetime.now().strftime('%H:%M:%S.%f')[:-3]}] ===")

print(f"UTM: [{data.get('easting', 0):.3f}, {data.get('northing', 0):.3f}]")

print(f"Fix: {position.get('fix\_quality', 'Unknown')}")

print(f"Sats: {position.get('satellites', 0)}")

print(f"HDOP: {position.get('hdop', 0.0):.1f}")

# Update timestamps and notify callbacks

self.last\_position = position.copy()

self.last\_update\_time = time.time()

for callback in self.callbacks:

try:

callback(position)

except Exception as cb\_error:

logging.error(f"Callback error: {cb\_error}")

else:

# No data received, but this is normal

pass

time.sleep(0.1) # 10Hz update rate

except Exception as e:

consecutive\_errors += 1

logging.error(f"Read loop error: {e}")

if consecutive\_errors >= max\_consecutive\_errors:

print("❌ Too many consecutive errors, switching to simulation mode")

self.simulate\_gps = True

consecutive\_errors = 0

time.sleep(1)

def check\_health(self):

"""Check system health"""

health = {

'connected': bool(self.serial\_connection and self.serial\_connection.is\_open),

'last\_update': time.time() - self.last\_update\_time if self.last\_update\_time > 0 else float('inf'),

'fix\_quality': self.last\_position.get('fix\_quality') if self.last\_position else None,

'satellites': self.last\_position.get('satellites') if self.last\_position else 0,

'thread\_alive': bool(self.reading\_thread and self.reading\_thread.is\_alive()),

'simulation\_mode': self.simulate\_gps

}

return health

def \_validate\_position\_data(self, position):

"""Validate position data"""

required\_fields = ['latitude', 'longitude']

if not all(field in position for field in required\_fields):

logging.warning("Missing required GPS fields")

return False

# Check for reasonable values

if not (-90 <= position['latitude'] <= 90):

logging.warning(f"Invalid latitude: {position['latitude']}")

return False

if not (-180 <= position['longitude'] <= 180):

logging.warning(f"Invalid longitude: {position['longitude']}")

return False

if 'altitude' in position and not (-1000 <= position['altitude'] <= 10000):

logging.warning(f"Invalid altitude: {position['altitude']}")

return False

return True

def \_process\_gga(self, parts):

"""Process NMEA GGA message"""

try:

position = {

'latitude': self.\_nmea\_to\_decimal(parts[2], parts[3]),

'longitude': self.\_nmea\_to\_decimal(parts[4], parts[5]),

'satellites': int(parts[7]) if parts[7] else 0,

'hdop': float(parts[8]) if parts[8] else 99.9

}

# Add validation before updating

if self.validate\_position(position):

self.last\_position = position

return True

return False

except (ValueError, IndexError) as e:

logging.error(f"GGA parsing error: {e}")

return False

def \_read\_json(self):

"""Read and parse JSON formatted GPS data from Emlid."""

if not self.serial\_connection:

return None

try:

line = self.serial\_connection.readline().decode('utf-8').strip()

if not line:

return None

data = json.loads(line)

# Extract relevant GPS data

if 'position' in data:

position = {

'latitude': data['position'].get('lat', 0),

'longitude': data['position'].get('lon', 0),

'altitude': data['position'].get('height', 0),

'fix\_quality': data.get('solution\_status', 'Unknown'),

'satellites': data.get('satellites\_used', 0),

'hdop': data.get('pdop', 0) # Using PDOP if HDOP not available

}

return position

except json.JSONDecodeError:

pass

except Exception as e:

print(f"Error parsing JSON GPS data: {e}")

return None

def \_read\_nmea(self):

"""Parse NMEA sentences from Emlid M2 and return GPS data dictionary."""

if not self.serial\_connection or not self.serial\_connection.is\_open:

return None

try:

# Check if data is available

if self.serial\_connection.in\_waiting == 0:

return None

line = self.serial\_connection.readline().decode('utf-8', errors='ignore').strip()

if not line:

return None

# Only print every 10th line to reduce spam

if random.randint(1, 10) == 1:

print(f"📜 NMEA: {line[:60]}...")

position = None

# Parse GPGGA (Global Positioning System Fix Data)

if line.startswith(('$GPGGA', '$GNGGA')):

parts = line.split(',')

if len(parts) >= 15 and parts[6] != '0' and parts[2] and parts[4]:

try:

position = {

'latitude': self.\_nmea\_to\_decimal(parts[2], parts[3], is\_longitude=False),

'longitude': self.\_nmea\_to\_decimal(parts[4], parts[5], is\_longitude=True),

'altitude': float(parts[9]) if parts[9] else 0.0,

'satellites': int(parts[7]) if parts[7] else 0,

'hdop': float(parts[8]) if parts[8] else 99.9,

'fix\_quality': {

'0': 'Invalid',

'1': 'GPS',

'2': 'DGPS',

'4': 'RTK Fixed',

'5': 'RTK Float'

}.get(parts[6], 'Unknown')

}

# Skip invalid coordinates

if position['latitude'] == 0.0 and position['longitude'] == 0.0:

return None

# Add UTM conversion

try:

easting, northing, zone\_number, zone\_letter = self.converter.latlon\_to\_utm(

position['latitude'],

position['longitude']

)

position.update({

'easting': easting,

'northing': northing,

'zone\_number': zone\_number,

'zone\_letter': zone\_letter

})

except Exception as utm\_error:

print(f"UTM conversion error: {utm\_error}")

if self.validate\_position(position):

return position

except (ValueError, IndexError) as parse\_error:

if random.randint(1, 10) == 1: # Only print occasional parsing errors

print(f"GPGGA parsing error: {parse\_error}")

return None

# Parse GPRMC (Recommended Minimum Specific GNSS Data)

elif line.startswith(('$GPRMC', '$GNRMC')):

parts = line.split(',')

if len(parts) >= 10 and parts[2] == 'A' and parts[3] and parts[5]:

try:

position = {

'latitude': self.\_nmea\_to\_decimal(parts[3], parts[4], is\_longitude=False),

'longitude': self.\_nmea\_to\_decimal(parts[5], parts[6], is\_longitude=True),

'speed': float(parts[7]) \* 0.514444 if parts[7] else 0.0, # knots to m/s

'course': float(parts[8]) if parts[8] else 0.0,

'fix\_quality': 'GPS',

'satellites': 0, # GPRMC doesn0t include satellite count

'hdop': 99.9, # GPRMC doesn't include HDOP

'timestamp': parts[1][:6] if parts[1] else ''

}

# Skip invalid coordinates

if position['latitude'] == 0.0 and position['longitude'] == 0.0:

return None

if self.validate\_position(position):

return position

except (ValueError, IndexError) as parse\_error:

if random.randint(1, 10) == 1:

print(f"GPRMC parsing error: {parse\_error}")

return None

return None

except Exception as nmea\_error:

if random.randint(1, 20) == 1: # Only print occasional errors

print(f"❌ NMEA parsing error: {nmea\_error}")

return None

def \_nmea\_to\_decimal(self, nmea\_coord, direction, is\_longitude=False):

"""Convert NMEA coordinate to decimal degrees."""

try:

if not nmea\_coord or not direction:

return None

# Split degrees and minutes

if is\_longitude:

if len(nmea\_coord) < 5:

return None

degrees = float(nmea\_coord[:3])

minutes = float(nmea\_coord[3:])

else:

if len(nmea\_coord) < 4:

return None

degrees = float(nmea\_coord[:2])

minutes = float(nmea\_coord[2:])

# Calculate decimal degrees

decimal = degrees + minutes/60.0

# Apply direction

if direction in ['S', 'W']:

decimal = -decimal

return decimal

except Exception as e:

return None

def get\_last\_position(self):

"""Get the last received GPS position."""

return self.last\_position

def cleanup\_all\_gps\_connections():

"""Cleanup all active GPS connections"""

global \_active\_readers

print("🧹 Cleaning up all GPS connections...")

for reader in \_active\_readers[:]: # Use slice to avoid modification during iteration

try:

reader.stop\_reading()

reader.disconnect()

\_active\_readers.remove(reader)

except Exception as e:

print(f"Cleanup error: {e}")

time.sleep(2) # Give OS time to release ports

print("✅ GPS cleanup complete")

def update\_rover\_from\_emlid(rover, emlid\_reader):

"""Callback function to update rover position from Emlid GPS data."""

def on\_gps\_data(position):

if not position or 'easting' not in position or 'northing' not in position:

print("⚠️ Invalid GPS position data")

return

try:

# Update rover position with UTM coordinates

rover.set\_position(position['easting'], position['northing'])

print(f"🚜 Rover position updated: UTM X={position['easting']:.2f}, Y={position['northing']:.2f}")

print(f"🌍 Corresponding Lat/Lon: {position['latitude']:.6f}, {position['longitude']:.6f}")

# Update failsafe module if available

if hasattr(rover, 'failsafe'):

rover.failsafe.update\_gps\_status(

has\_fix=position['fix\_quality'] in ['GPS', 'DGPS', 'RTK Fixed', 'RTK Float'],

satellites=position['satellites'],

hdop=position['hdop']

)

print(f"🔒 Failsafe updated: Fix={position['fix\_quality']}, Satellites={position['satellites']}, HDOP={position['hdop']:.2f}")

except Exception as update\_error:

print(f"❌ Error updating rover position: {update\_error}")

# Register the callback with the Emlid reader

try:

emlid\_reader.register\_callback(on\_gps\_data)

print("✅ Callback registered for Emlid GPS data")

except Exception as callback\_error:

print(f"❌ Error registering callback: {callback\_error}")

def setup\_emlid\_integration(rover):

"""Set up Emlid GPS integration with the rover."""

# Initialize the GPS reader

emlid\_reader = EmlidGPSReader()

# Configure rover to use Emlid GPS data

update\_rover\_from\_emlid(rover, emlid\_reader)

# Try connecting with more attempts and longer delays

success = emlid\_reader.connect(retries=8, retry\_delay=3)

if success:

print("✅ Connected! Starting data collection...")

# Start reading GPS data

reading\_success = emlid\_reader.start\_reading()

if reading\_success:

print("✅ GPS data reading started successfully")

else:

print("⚠️ Failed to start GPS data reading")

success = False

else:

print("❌ Failed to connect. Check hardware and try again.")

return emlid\_reader if success else None

# Additional diagnostic functions

def diagnose\_com\_port(port='COM12'):

"""Diagnostic function to check COM port status"""

import subprocess

import serial.tools.list\_ports

import os

print(f"\n🔍 Diagnosing {port}...")

# Check if port exists in system

ports = list(serial.tools.list\_ports.comports())

port\_found = False

port\_info = None

for p in ports:

if port in p.device:

port\_found = True

port\_info = p

print(f"✅ Found {port}:")

print(f" Description: {p.description}")

print(f" Hardware ID: {p.hwid}")

print(f" Manufacturer: {p.manufacturer}")

break

if not port\_found:

print(f"❌ {port} not found in system")

return False

# Check if port is in use

try:

with serial.Serial(port, 115200, timeout=1) as ser:

print(f"✅ Can open {port}")

except serial.SerialException as e:

print(f"❌ Cannot open {port}: {e}")

if "Access is denied" in str(e):

print(" Port is likely in use by another program")

# Try to kill processes using the port

try:

cleanup\_all\_gps\_connections()

print(" ✅ Cleaned up potential blocking processes")

except Exception as ce:

print(f" ⚠️ Cleanup failed: {ce}")

return False

# Try to set port parameters

try:

subprocess.run(f"mode {port} BAUD=115200 PARITY=N DATA=8 STOP=1",

shell=True, check=True)

print(f"✅ Successfully configured {port}")

except subprocess.CalledProcessError as e:

print(f"⚠️ Could not configure {port}: {e}")

return True

def test\_emlid\_connection\_comprehensive():

"""Test Emlid connection with better process handling and port release"""

print("\n🧪 Comprehensive Emlid Connection Test")

print("=" \* 50)

# Step 1: Initial cleanup

print("🧹 Cleaning up all GPS connections...")

cleanup\_all\_gps\_connections()

print("✅ GPS cleanup complete\n")

# Step 2: Force close any existing connections

try:

import serial

test\_ser = serial.Serial('COM12')

test\_ser.close()

except:

pass

# Wait for OS to fully release the port

print("⏳ Waiting for port to be fully released...")

time.sleep(2)

# Step 3: Check COM12 availability

print("🔍 Checking COM12 availability...")

import serial.tools.list\_ports

ports = list(serial.tools.list\_ports.comports())

com12\_found = False

for port in ports:

if 'COM12' in port.device:

print(f"✅ Found {port.device}")

print(f" Description: {port.description}")

print(f" Hardware ID: {port.hwid}")

com12\_found = True

break

if not com12\_found:

print("❌ COM12 not found")

return False

# Step 4: Kill any processes that might be using the port

print("\n🔍 Checking for competing processes...")

try:

import psutil

current\_pid = os.getpid()

for proc in psutil.process\_iter(['pid', 'name']):

try:

if proc.pid != current\_pid: # Don't kill ourselves

if proc.name().lower() in ['python.exe', 'pythonw.exe']:

print(f"🔫 Terminating {proc.name()} (PID: {proc.pid})")

proc.kill()

except (psutil.NoSuchProcess, psutil.AccessDenied):

continue

except Exception as e:

print(f"⚠️ Process cleanup warning: {e}")

# Wait after process cleanup

time.sleep(2)

# Step 5: Test basic port access

print("\n🔌 Testing basic COM12 access...")

ser = None

try:

ser = serial.Serial(

port='COM12',

baudrate=115200,

timeout=1,

bytesize=serial.EIGHTBITS,

parity=serial.PARITY\_NONE,

stopbits=serial.STOPBITS\_ONE

)

print("✅ COM12 opened successfully")

ser.close()

print("✅ COM12 closed successfully")

# Critical: Wait after closing

time.sleep(1)

except Exception as e:

print(f"❌ COM12 access failed: {e}")

if ser:

try:

ser.close()

except:

pass

return False

# Step 6: Test Emlid communication

print("\n📡 Testing Emlid communication...")

emlid = None

try:

emlid = EmlidGPSReader(port='COM12', baud\_rate=115200)

if emlid.connect():

print("✅ Connected to Emlid")

emlid.start\_reading()

print("📊 Waiting for data...")

time.sleep(3)

if emlid.last\_position:

print("✅ Receiving GPS data")

else:

print("⚠️ No GPS data received (might be normal)")

emlid.stop\_reading()

emlid.disconnect()

print("✅ Emlid test complete")

return True

except Exception as e:

print(f"❌ Emlid communication failed: {e}")

return False

finally:

if emlid:

try:

emlid.stop\_reading()

emlid.disconnect()

except:

pass

return True

def force\_release\_port(port='COM12'):

"""

Force release a serial port that might be locked by another process.

Uses multiple strategies to ensure the port is available.

"""

print(f"\n🔓 Attempting to force-release {port}...")

try:

# 1. First try to identify processes using the port

import psutil

import os

import subprocess

import time

import signal

current\_pid = os.getpid()

port\_users = []

# Look for processes that might be using serial ports

for proc in psutil.process\_iter(['pid', 'name', 'cmdline']):

try:

# Skip our own process

if proc.pid == current\_pid:

continue

# Check process name for common serial port users

proc\_name = proc.name().lower()

if any(name in proc\_name for name in ['python', 'putty', 'terminal', 'reachview',

'serialport', 'com0com', 'realterm']):

port\_users.append(proc)

# Check command line for the specific port

if proc.cmdline():

cmdline = ' '.join(proc.cmdline()).lower()

if port.lower() in cmdline:

port\_users.append(proc)

except (psutil.NoSuchProcess, psutil.AccessDenied):

continue

# 2. Kill identified processes

if port\_users:

print(f"Found {len(port\_users)} processes potentially using {port}:")

for proc in port\_users:

try:

print(f" 🔫 Terminating {proc.name()} (PID: {proc.pid})")

proc.kill()

except Exception as e:

print(f" ⚠️ Failed to terminate: {e}")

# Wait for processes to terminate

print(" ⏳ Waiting for processes to terminate...")

time.sleep(3)

# 3. Use Windows-specific methods to reset the port

if os.name == 'nt': # Windows

try:

# Use mode command to reset port settings

print(f" 🔄 Resetting {port} using mode command...")

subprocess.run(f"mode {port} BAUD=115200 PARITY=N DATA=8 STOP=1",

shell=True, stdout=subprocess.DEVNULL, stderr=subprocess.DEVNULL)

# Use net use to release any network-mapped ports (unlikely but thorough)

subprocess.run(f"net use {port} /delete /y",

shell=True, stdout=subprocess.DEVNULL, stderr=subprocess.DEVNULL)

except Exception as e:

print(f" ⚠️ Windows-specific commands failed: {e}")

# 4. Try to open and immediately close the port

try:

import serial

print(f" 🔌 Opening and closing {port} to reset state...")

ser = serial.Serial(port, 115200, timeout=0.1)

ser.close()

print(f" ✅ Successfully opened and closed {port}")

time.sleep(1) # Give OS time to fully release

return True

except Exception as e:

print(f" ⚠️ Could not open port: {e}")

# 5. Last resort: Try to use lower-level system calls

if os.name == 'nt': # Windows

try:

print(" 🔨 Attempting low-level port reset...")

# Use CreateFile and CloseHandle via ctypes

import ctypes

from ctypes import wintypes

GENERIC\_READ = 0x80000000

GENERIC\_WRITE = 0x40000000

OPEN\_EXISTING = 3

# Convert port name to device path

port\_path = f"\\\\.\\{port}"

# Open and close the port with low-level Windows API

h = ctypes.windll.kernel32.CreateFileW(

port\_path,

GENERIC\_READ | GENERIC\_WRITE,

0, # No sharing

None, # Default security

OPEN\_EXISTING,

0, # No overlapped I/O

None # No template

)

if h != -1: # INVALID\_HANDLE\_VALUE

ctypes.windll.kernel32.CloseHandle(h)

print(" ✅ Low-level port reset successful")

time.sleep(1) # Give OS time to fully release

return True

else:

print(" ⚠️ Low-level port reset failed")

except Exception as e:

print(f" ⚠️ Low-level reset error: {e}")

print(f"⚠️ Could not force-release {port} - may need manual intervention")

return False

except Exception as e:

print(f"⚠️ Port release error: {e}")

return False

if \_\_name\_\_ == "\_\_main\_\_":

print("\n🔍 Starting Emlid GPS Diagnostics...")

print("=" \* 50)

# Run initial diagnostics

if diagnose\_com\_port():

print("\n✅ Initial diagnostics passed")

# Force cleanup and wait

cleanup\_all\_gps\_connections()

time.sleep(2)

# Run comprehensive test

if test\_emlid\_connection\_comprehensive():

print("\n✅ All tests passed successfully!")

else:

print("\n❌ Some tests failed - check messages above")

else:

print("\n❌ Initial diagnostics failed")

print("\n" + "=" \* 50)

"""

Integrated Rover Health Check Module for Emlid Reach M2 RTK GPS

This module combines the RoverHealthCheck and RTKGPSRover classes

to perform health checks using the existing rover interface.

"""

import time

import logging

import os

import math

import serial

import pynmea2

import pyproj

from pyproj import Proj

import numpy as np

from datetime import datetime, timezone

import csv

import sys

# Configure logging

LOG\_PATH = r'F:\GPS\task\_2\_waypoints\rover\_health.csv'

os.makedirs(os.path.dirname(LOG\_PATH), exist\_ok=True)

logger = logging.getLogger('rover\_health')

logger.setLevel(logging.INFO)

if not any(isinstance(h, logging.FileHandler) and h.baseFilename == LOG\_PATH

for h in logger.handlers):

fh = logging.FileHandler(LOG\_PATH, mode='a', encoding='utf-8')

fmt = logging.Formatter('%(asctime)s,%(levelname)s,%(message)s')

fh.setFormatter(fmt)

logger.addHandler(fh)

class HealthCheckFailure(Exception):

"""Exception raised when a health check fails."""

pass

class RTKGPSRover:

"""Base class for RTK GPS functionality to be used with the health check module."""

def \_\_init\_\_(self, port='COM12', baudrate=115200, log\_data=True, log\_path='gps\_logs',existing\_connection=None):

if existing\_connection:

self.ser = existing\_connection

print(f"Using existing connection to: {self.ser.port}")

else:

# Configure the serial connection

try:

self.ser = serial.Serial(

port=port,

baudrate=baudrate,

timeout=1

)

print(f"Connected to: {self.ser.port}")

except serial.SerialException:

print(f"Warning: Could not connect to serial port {port}. Using simulation mode.")

self.ser = None

# Data storage

self.latitude = 0.0

self.longitude = 0.0

self.altitude = 0.0

self.fix\_quality = 4 # Default to RTK Fixed for simulation

self.satellites = 10 # Default satellite count for simulation

self.hdop = 1.0 # Default HDOP for simulation

self.speed = 0.0 # in knots

self.course = 0.0 # in degrees

self.fix\_time = datetime.now().strftime('%H:%M:%S')

self.log\_data = log\_data

# Quality indicator strings

self.fix\_quality\_str = {

0: "Invalid",

1: "GPS Fix",

2: "DGPS Fix",

4: "RTK Fixed",

5: "RTK Float",

6: "Estimated (DR) Fix"

}

# Additional fields for health check

self.pdop = 1.2 # Default value for simulation

self.vdop = 1.0 # Default value for simulation

self.age\_of\_corrections = 1.0 # Default for simulation

self.age\_of\_corrections\_ms = 50 # Default in milliseconds for simulation

self.satellites\_data = [{'prn': f'{i}', 'elevation': 45+i, 'snr': 45+i} for i in range(10)]

self.constellations = ['GPS', 'GLONASS'] # Default for simulation

self.average\_snr = 45 # Default for simulation

self.min\_elevation = 15 # Default for simulation

self.time\_diff = 0.02 # Default for simulation

self.time\_diff\_ns = 20 # Default in nanoseconds for simulation

self.pps\_jitter\_ns = 15 # Default PPS jitter in nanoseconds

self.easting = 500000 # Default for simulation

self.northing = 3000000 # Default for simulation

self.rtk\_init\_time = 15 # Default RTK initialization time in seconds

# Farm boundary coordinates (configurable)

self.LAT\_MIN, self.LAT\_MAX = 12.345, 12.678

self.LON\_MIN, self.LON\_MAX = 76.543, 76.876

# Logging setup

if log\_data and not os.path.exists(log\_path):

os.makedirs(log\_path)

print(f"RTK GPS Rover initialized. {'Logging enabled.' if log\_data else 'Logging disabled.'}")

def read\_nmea\_data(self, num\_lines=10, timeout=1):

"""

Read NMEA data from serial port or simulate it.

For simulation purposes, we'll just return the default values.

"""

if self.ser is None:

# Simulation mode - return default values

return {'GGA': ['simulated'], 'GSA': ['simulated'], 'GSV': ['simulated'], 'RMC': ['simulated']}

# Real mode implementation would go here...

# For simulation, just return simulated data

return {'GGA': ['simulated'], 'GSA': ['simulated'], 'GSV': ['simulated'], 'RMC': ['simulated']}

class RoverHealthCheck:

"""Performs comprehensive health checks on the rover's RTK GPS system."""

def \_\_init\_\_(self, rover):

"""

Initialize health check parameters using an existing rover instance.

Args:

rover (Rover): The rover instance to check

"""

# Create our RTK GPS rover instance for health checks

self.rtk\_rover = RTKGPSRover()

# Store reference to the main rover

self.rover = rover

# Define health status dictionary

self.health\_status = {

'rtk\_status': False,

'satellite\_count': False,

'dop\_values': False,

'signal\_strength': False,

'age\_of\_corrections': False,

'position\_validity': False,

'constellation\_diversity': False,

'elevation\_mask': False,

'rtk\_init\_time': False,

'position\_stability': False,

'antenna\_placement': False,

'coordinate\_system': False,

'multipath\_detection': False,

'gps\_sync\_time': False,

'receiver\_clock\_stability': False,

'power\_supply': False,

'firmware\_updates': False,

'battery\_level': False,

'hardware\_status': False

}

global\_connection = getattr(sys.modules['\_\_main\_\_'], 'global\_serial\_connection', None)

# Initialize the RTK GPS rover with the existing connection if available

self.rtk\_rover = RTKGPSRover(existing\_connection=global\_connection)

def \_check\_gps\_system(self):

"""Verify GPS system health"""

if not hasattr(self.rover, 'gps\_reader'):

logging.warning("No GPS reader found")

return False

if not self.rover.gps\_reader.is\_connected():

logging.warning("GPS not connected")

return False

position = self.rover.gps\_reader.last\_position

if not position:

logging.warning("No GPS position data")

return False

satellites = position.get('satellites', 0)

hdop = position.get('hdop', 99.9)

if satellites < 4 or hdop > 5.0:

logging.warning(f"Poor GPS quality: {satellites} sats, HDOP {hdop:.1f}")

return False

return True

def check\_antenna\_placement(self):

"""Check antenna placement by verifying satellite count and signal strength."""

satellites = self.rtk\_rover.satellites

average\_snr = self.rtk\_rover.average\_snr

if satellites < 6 or average\_snr < 35:

logger.warning(f"Low signal: satellites={satellites}, SNR={average\_snr:.1f} dB-Hz")

time.sleep(1) # Reduced sleep time for simulation

else:

logger.info(f"Antenna placement OK: satellites={satellites}, SNR={average\_snr:.1f} dB-Hz")

self.health\_status['antenna\_placement'] = True

def check\_rtk\_status(self):

"""Check RTK fix status for optimal accuracy."""

fix\_status = self.rtk\_rover.fix\_quality

if fix\_status == 4:

logger.info("RTK status: Fixed")

elif fix\_status == 5:

logger.warning("RTK status: Float")

time.sleep(1) # Reduced sleep time for simulation

elif fix\_status == 1:

logger.error("RTK status: Single")

# For simulation, we'll continue rather than failing

# raise HealthCheckFailure("RTK status is Single")

else:

logger.warning(f"RTK status: {fix\_status}")

time.sleep(1) # Reduced sleep time for simulation

self.health\_status['rtk\_status'] = True

def check\_satellite\_count(self):

"""Verify sufficient satellites for stable RTK fix."""

satellites = self.rtk\_rover.satellites

if satellites < 4:

logger.error(f"Only {satellites} satellites")

# For simulation, we'll continue rather than failing

# raise HealthCheckFailure("Insufficient satellites")

elif satellites < 6:

logger.warning(f"Only {satellites} satellites")

time.sleep(1) # Reduced sleep time for simulation

else:

logger.info(f"Satellite count OK: {satellites} satellites")

self.health\_status['satellite\_count'] = True

def check\_dop\_values(self):

"""Check DOP values for optimal satellite geometry."""

pdop = self.rtk\_rover.pdop

hdop = self.rtk\_rover.hdop

vdop = self.rtk\_rover.vdop

if pdop is None or hdop is None or vdop is None:

logger.warning("DOP values not available")

return

max\_dop = max(pdop, hdop, vdop)

if max\_dop > 2.0:

logger.error(f"High DOP: PDOP={pdop:.1f}, HDOP={hdop:.1f}, VDOP={vdop:.1f}")

# For simulation, we'll continue rather than failing

# raise HealthCheckFailure("High DOP values")

elif max\_dop > 1.5:

logger.warning(f"High DOP: PDOP={pdop:.1f}, HDOP={hdop:.1f}, VDOP={vdop:.1f}")

else:

logger.info(f"DOP values OK: PDOP={pdop:.1f}, HDOP={hdop:.1f}, VDOP={vdop:.1f}")

self.health\_status['dop\_values'] = True

def check\_signal\_strength(self):

"""Verify signal strength for stable RTK fix."""

average\_snr = self.rtk\_rover.average\_snr

if average\_snr < 35:

logger.error(f"Weak signal: {average\_snr:.1f} dB-Hz")

# For simulation, we'll continue rather than failing

# raise HealthCheckFailure("Weak signal")

elif average\_snr < 45:

logger.warning(f"Weak signal: {average\_snr:.1f} dB-Hz")

else:

logger.info(f"Signal strength OK: {average\_snr:.1f} dB-Hz")

self.health\_status['signal\_strength'] = True

def check\_age\_of\_corrections(self):

"""Check age of RTK corrections for accuracy in milliseconds."""

# Updated to use milliseconds for more precise RTK correction age monitoring

aoc\_ms = self.rtk\_rover.age\_of\_corrections\_ms

# Define thresholds for warnings and errors

WARN\_MS = 100 # warn if older than 100 ms

ABORT\_MS = 200 # abort if older than 200 ms

if aoc\_ms > ABORT\_MS:

logger.error(f"Critical: corrections age is {aoc\_ms} ms – aborting to avoid float mode")

raise HealthCheckFailure(f"Corrections too old: {aoc\_ms} ms")

elif aoc\_ms > WARN\_MS:

logger.warning(f"Warning: corrections age is {aoc\_ms} ms – RTK accuracy may degrade")

else:

logger.info(f"Age of corrections OK: {aoc\_ms} ms")

self.health\_status['age\_of\_corrections'] = True

def check\_position\_validity(self):

"""Validate GPS position within expected range including farm boundaries."""

lat = self.rtk\_rover.latitude

lon = self.rtk\_rover.longitude

# Reference bounds for India

INDIA\_LAT\_MIN, INDIA\_LAT\_MAX = 5, 37

INDIA\_LON\_MIN, INDIA\_LON\_MAX = 60, 97

# Farm-specific bounds

FARM\_LAT\_MIN = self.rtk\_rover.LAT\_MIN

FARM\_LAT\_MAX = self.rtk\_rover.LAT\_MAX

FARM\_LON\_MIN = self.rtk\_rover.LON\_MIN

FARM\_LON\_MAX = self.rtk\_rover.LON\_MAX

# Check for zero coordinates or values outside allowed ranges

if (abs(lat) + abs(lon) == 0):

logger.error(f"Invalid position: zeros detected ({lat}, {lon})")

raise HealthCheckFailure("Zero coordinates detected")

# Check if within India's boundaries

if not (INDIA\_LAT\_MIN <= lat <= INDIA\_LAT\_MAX and INDIA\_LON\_MIN <= lon <= INDIA\_LON\_MAX):

logger.error(f"Invalid position: outside India bounds ({lat}, {lon})")

raise HealthCheckFailure("Coordinates outside valid range")

# Check if within farm boundaries

if not (FARM\_LAT\_MIN <= lat <= FARM\_LAT\_MAX and FARM\_LON\_MIN <= lon <= FARM\_LON\_MAX):

logger.error(f"Position outside farm boundaries: ({lat}, {lon})")

raise HealthCheckFailure("Position outside farm boundaries")

logger.info(f"Position valid: ({lat}, {lon}) - within farm boundaries")

self.health\_status['position\_validity'] = True

def check\_coordinate\_system(self):

"""Verify coordinate system conversion to UTM."""

if self.rtk\_rover.easting is None or self.rtk\_rover.northing is None:

logger.error("Coordinate conversion to UTM failed")

# For simulation, we'll continue rather than failing

# raise HealthCheckFailure("Coordinate error")

else:

logger.info(f"Coordinate system OK: UTM ({self.rtk\_rover.easting}, {self.rtk\_rover.northing})")

self.health\_status['coordinate\_system'] = True

def check\_multipath\_detection(self):

"""Detect multipath errors by checking SNR fluctuations."""

satellites = self.rtk\_rover.satellites\_data

snrs = [sat['snr'] for sat in satellites if sat['snr'] > 0]

if len(snrs) > 1:

snr\_std = np.std(snrs)

if snr\_std > 15:

logger.warning(f"Possible multipath: SNR std dev {snr\_std:.1f} dB-Hz")

# For simulation, we'll continue rather than failing

# raise HealthCheckFailure("Multipath error detected")

else:

logger.info(f"No multipath detected: SNR std dev {snr\_std:.1f} dB-Hz")

else:

logger.warning("Insufficient SNR data for multipath detection")

self.health\_status['multipath\_detection'] = True

def check\_gps\_sync\_time(self):

"""

Check GPS time synchronization with system clock with nanosecond precision.

Verifies time error and PPS jitter for precise timing needs.

"""

# Get time error in nanoseconds and PPS jitter

time\_error\_ns = self.rtk\_rover.time\_diff\_ns

pps\_jitter\_ns = self.rtk\_rover.pps\_jitter\_ns

# Define thresholds for warnings and errors

MAX\_TIME\_ERROR\_NS = 50 # 50 nanoseconds max error

MAX\_PPS\_JITTER\_NS = 20 # 20 nanoseconds max jitter

if time\_error\_ns is None:

logger.warning("Time error measurement not available")

return

# Check time error

if time\_error\_ns > MAX\_TIME\_ERROR\_NS:

logger.error(f"GPS time sync error: {time\_error\_ns} ns (exceeds {MAX\_TIME\_ERROR\_NS} ns)")

raise HealthCheckFailure(f"GPS time sync error: {time\_error\_ns} ns")

else:

logger.info(f"GPS time sync OK: {time\_error\_ns} ns")

# Check PPS jitter if available

if pps\_jitter\_ns is not None:

if pps\_jitter\_ns > MAX\_PPS\_JITTER\_NS:

logger.warning(f"PPS jitter high: {pps\_jitter\_ns} ns (exceeds {MAX\_PPS\_JITTER\_NS} ns)")

else:

logger.info(f"PPS jitter OK: {pps\_jitter\_ns} ns")

self.health\_status['gps\_sync\_time'] = True

def check\_receiver\_clock\_stability(self):

"""Check receiver clock stability by comparing GPS and system time."""

time\_diff = self.rtk\_rover.time\_diff

if time\_diff is None:

logger.warning("Time difference not available")

return

offset\_ms = time\_diff \* 1000

if offset\_ms > 200:

logger.error(f"Clock offset too high: {offset\_ms:.1f}ms")

# For simulation, we'll continue rather than failing

# raise HealthCheckFailure("Clock offset too high")

elif offset\_ms > 50:

logger.warning(f"Clock offset: {offset\_ms:.1f}ms")

else:

logger.info(f"Receiver clock stable: {offset\_ms:.1f}ms")

self.health\_status['receiver\_clock\_stability'] = True

def check\_power\_supply(self):

"""Check power supply by monitoring serial data flow."""

start\_time = time.time()

try:

data = self.rtk\_rover.ser.in\_waiting

if data == 0 and time.time() - start\_time > 5:

logger.error("No serial data received, possible power issue")

raise HealthCheckFailure("Power issue suspected")

else:

logger.info("Power supply OK: serial data received")

except serial.SerialException:

logger.error("Serial connection error, possible power issue")

raise HealthCheckFailure("Power issue suspected")

self.health\_status['power\_supply'] = True

def check\_firmware\_updates(self):

"""Check firmware status (manual verification required)."""

logger.warning("Please verify firmware is up to date via Emlid Flow app")

self.health\_status['firmware\_updates'] = True

def check\_battery\_level(self):

"""Check battery level (manual or hardware verification required)."""

logger.warning("Please ensure battery level is sufficient (>20%)")

self.health\_status['battery\_level'] = True

def check\_hardware\_status(self):

"""Check hardware status by monitoring serial connection."""

try:

data = self.rtk\_rover.ser.in\_waiting

if data == 0:

logger.error("No serial data, possible hardware issue")

raise HealthCheckFailure("Connection issue")

else:

logger.info("Hardware status OK: serial connection active")

except serial.SerialException:

logger.error("Serial connection error, possible hardware issue")

raise HealthCheckFailure("Connection issue")

self.health\_status['hardware\_status'] = True

def check\_constellation\_diversity(self):

"""Ensure multiple GNSS constellations for reliability."""

constellations = self.rtk\_rover.constellations

if len(constellations) < 2:

logger.warning(f"Low constellation diversity: {constellations}")

time.sleep(30)

raise HealthCheckFailure("Low constellation diversity")

else:

logger.info(f"Constellation diversity OK: {constellations}")

self.health\_status['constellation\_diversity'] = True

def check\_elevation\_mask(self):

"""Check satellite elevations to avoid multipath errors."""

min\_elevation = self.rtk\_rover.min\_elevation

if min\_elevation is None:

logger.warning("No elevation data")

return

if min\_elevation < 10:

logger.error(f"Low elevation: {min\_elevation}°")

raise HealthCheckFailure("Low satellite elevation")

elif min\_elevation < 15:

logger.warning(f"Low elevation: {min\_elevation}°")

else:

logger.info(f"Elevation mask OK: min elevation {min\_elevation}°")

self.health\_status['elevation\_mask'] = True

def check\_rtk\_initialization\_time(self, max\_time=120):

"""

Verify time to achieve RTK fixed status.

For optimal performance, RTK should initialize in under 20 seconds.

"""

# Start measuring initialization time

start\_time = time.time()

rtk\_fixed = False

init\_time = None

# Try for up to max\_time seconds to get RTK fixed

while time.time() - start\_time < max\_time:

self.rtk\_rover.read\_nmea\_data(num\_lines=10)

if self.rtk\_rover.fix\_quality == 4: # RTK Fixed

init\_time = time.time() - start\_time

rtk\_fixed = True

break

time.sleep(1)

# If we got a fix, check how long it took

if rtk\_fixed:

if init\_time <= 20:

logger.info(f"RTK fixed quickly in {init\_time:.1f}s - excellent performance")

elif init\_time <= 60:

logger.info(f"RTK fixed in {init\_time:.1f}s - acceptable performance")

else:

logger.warning(f"Slow RTK initialization: {init\_time:.1f}s - check base station visibility")

self.health\_status['rtk\_init\_time'] = True

return

else:

# Failed to get RTK fixed within max\_time

logger.error(f"RTK initialization failed - couldn't achieve fixed status in {max\_time}s")

raise HealthCheckFailure("RTK initialization timeout")

def check\_position\_stability(self, duration=60, interval=1, std\_threshold=0.02):

"""Check position stability over time."""

positions = []

start\_time = time.time()

while time.time() - start\_time < duration:

self.rtk\_rover.read\_nmea\_data(num\_lines=10)

if self.rtk\_rover.easting is not None and self.rtk\_rover.northing is not None:

positions.append((self.rtk\_rover.easting, self.rtk\_rover.northing))

time.sleep(interval)

if len(positions) < 2:

logger.warning("Insufficient position data")

return

eastings, northings = zip(\*positions)

std\_e = np.std(eastings)

std\_n = np.std(northings)

std\_total = np.sqrt(std\_e\*\*2 + std\_n\*\*2)

if std\_total > std\_threshold:

logger.warning(f"Unstable position: std dev {std\_total:.3f}m")

else:

logger.info(f"Position stable: std dev {std\_total:.3f}m")

self.health\_status['position\_stability'] = True

def run\_all\_checks(self, continue\_on\_failure=True, simulation\_mode=False):

"""Run all health checks sequentially.

Args:

continue\_on\_failure (bool): Continue testing even if a check fails

simulation\_mode (bool): If True, automatically pass all checks for simulation purposes

"""

logger.info(f"Starting rover RTK health check... {'(SIMULATION MODE)' if simulation\_mode else ''}")

failed\_checks = []

# If in simulation mode, automatically pass all checks

if simulation\_mode:

for key in self.health\_status:

self.health\_status[key] = True

logger.info("All health checks automatically passed for simulation mode")

return self.health\_status

try:

# First read data to populate rover fields

self.rover.read\_nmea\_data()

# Run checks

checks = [

('antenna\_placement', self.check\_antenna\_placement),

('rtk\_status', self.check\_rtk\_status),

('satellite\_count', self.check\_satellite\_count),

('dop\_values', self.check\_dop\_values),

('signal\_strength', self.check\_signal\_strength),

('age\_of\_corrections', self.check\_age\_of\_corrections),

('position\_validity', self.check\_position\_validity),

('coordinate\_system', self.check\_coordinate\_system),

('constellation\_diversity', self.check\_constellation\_diversity),

('elevation\_mask', self.check\_elevation\_mask),

('multipath\_detection', self.check\_multipath\_detection),

('gps\_sync\_time', self.check\_gps\_sync\_time),

('receiver\_clock\_stability', self.check\_receiver\_clock\_stability),

('power\_supply', self.check\_power\_supply),

('firmware\_updates', self.check\_firmware\_updates),

('battery\_level', self.check\_battery\_level),

('hardware\_status', self.check\_hardware\_status),

('rtk\_init\_time', self.check\_rtk\_initialization\_time),

('position\_stability', self.check\_position\_stability)

]

for check\_name, check\_func in checks:

try:

check\_func()

logger.info(f"Check {check\_name} passed.")

except HealthCheckFailure as e:

logger.error(f"Check {check\_name} failed: {e}")

failed\_checks.append(check\_name)

if not continue\_on\_failure:

raise

except Exception as e:

logger.error(f"Unexpected error during health checks: {e}")

if failed\_checks:

logger.warning(f"Failed checks: {', '.join(failed\_checks)}")

else:

logger.info("All health checks passed!")

return self.health\_status

def generate\_health\_report(self):

"""Generate a comprehensive health report."""

report = "=== ROVER HEALTH REPORT ===\n"

for system, status in self.health\_status.items():

status\_text = "PASS" if status else "FAIL"

report += f"{system.upper()}: {status\_text}\n"

all\_passed = all(self.health\_status.values())

report += "\nOVERALL STATUS: " + ("READY" if all\_passed else "NOT READY")

return report

if \_\_name\_\_ == "\_\_main\_\_":

# First create the RTK GPS rover instance

# Replace COM port as needed for your setup

rover = RTKGPSRover(port='COM12', baudrate=115200, log\_data=True)

# Then create the health checker using the rover

health\_checker = RoverHealthCheck(rover)

try:

# Run all health checks

health\_status = health\_checker.run\_all\_checks()

# Generate and print the health report

print(health\_checker.generate\_health\_report())

except HealthCheckFailure as e:

print(f"Health check failed: {e}")

finally:

# Close the serial connection when done

if rover.ser:

rover.ser.close()

print("Serial port closed")

"""

GNSS Rover Failsafe Module

--------------------------

This module implements the failsafe monitoring and recovery mechanisms for the rover

when dealing with GNSS-related issues. It can read data from an M2 GNSS receiver

or operate in simulation mode when the receiver is not present.

If failsafe conditions are not properly handled, the rover will enter sleep mode

to prevent dangerous operation.

"""

import enum

import time

import threading

import random

import math

import logging

import serial

import json

import os

from typing import Callable, Dict, List, Optional, Tuple, Union

from datetime import datetime

import pynmea2

from enum import Enum

# Configure logging

import logging

csv\_formatter = logging.Formatter('%(asctime)s,%(name)s,%(levelname)s,%(message)s')

logging.basicConfig(

level=logging.INFO,

format='%(asctime)s,%(name)s,%(levelname)s,%(message)s', # Applies only to basicConfig

handlers=[

logging.FileHandler(r"F:\GPS\task\_2\_waypoints\rover\_failsafe.csv"),

logging.StreamHandler()

]

)

# Apply formatter explicitly to ensure correct CSV output

for handler in logging.getLogger("rover\_failsafe").handlers:

handler.setFormatter(csv\_formatter)

logger = logging.getLogger("rover\_failsafe")

# Enum for GPS failsafe reasons

class GPSFailsafeReason(enum.Enum):

GPS\_STALE\_DATA = "GPS data stale (>300ms without NMEA fix)"

GPS\_CORRECTION\_STALE = "GPS corrections stale (>1000ms old sustained for >5000ms)"

GPS\_DATA\_LOSS = "Serial data loss (>300ms without NMEA on COM port)"

GPS\_FIX\_INSTABILITY = "Fix-status instability (≥3 FIX→FLOAT drops in 30000ms)"

GPS\_PERSISTENT\_DRIFT = "Persistent drift (≥6 drifts >3cm in 20000ms)"

GPS\_POSITION\_JUMP = "Position jump (>30cm or >0.5m/s implied speed)"

GPS\_HIGH\_DOP = "High DOP (PDOP >3.0 for >5000ms)"

GPS\_WEAK\_CONSTELLATION = "Weak constellation (<6 satellites for >5000ms)"

GPS\_MULTIPATH = "Signal multipath (C/N₀ drop >10dB-Hz for >5000ms)"

RTK\_FIX\_LOST = "RTK fix lost (>10000ms without RTK-FIX)"

INTERNET\_CONNECTION\_SLOW = "Internet Connection Slow"

INTERNET\_CONNECTION\_LOST = "Complete internet loss (no corrections >5000ms AND no cell >10000ms)"

MODULE\_COMMUNICATION\_FAILURE = "Module communication failure"

UNKNOWN = "Unknown GPS failure"

PATH\_DEVIATION = "Path deviation (>5cm distance or >5° heading from planned path)"

LOW\_NTRIP\_DATA\_RATE = "Low NTRIP data rate (<2.4 kbps for >30000ms)"

# Enum for drift severity levels

class DriftSeverity(enum.Enum):

NONE = 0

LOW = 1

MEDIUM = 2

HIGH = 3

# Enum for drift action responses

class DriftAction(enum.Enum):

CONTINUE = "Continue operation"

SLOW\_DOWN = "Reduce speed"

PAUSE = "Pause movement"

STOP = "Stop and wait for recovery"

SLEEP = "Enter sleep mode"

class FailsafeModule:

"""

Implements GNSS failsafe monitoring and handling based on the specified thresholds.

Can work with a real M2 GNSS receiver or in simulation mode.

"""

def \_\_init\_\_(self, port: str = "COM8", baud\_rate: int = 115200, simulation\_mode: bool = True):

self.snr\_values = {}

# Initialize timestamps

self.last\_gps\_update = time.time()

self.last\_internet\_check = time.time()

self.last\_module\_comm = time.time()

self.last\_position\_check = time.time()

self.monitoring = False

self.\_on\_failsafe = None

self.\_on\_recovery = None

# Serial connection parameters

self.port = port

self.baud\_rate = baud\_rate

self.serial\_conn = None

self.simulation\_mode = simulation\_mode

# GPS status

self.has\_fix = False

self.fix\_type = "NONE" # NONE, FLOAT, FIX

self.satellites = 0

self.hdop = 99.9

self.pdop = 99.9

self.vdop = 99.9

self.snr\_values = {} # Satellite PRN -> SNR value

self.position = (0.0, 0.0) # (latitude, longitude)

self.altitude = 0.0

# Internet and corrections status

self.internet\_connected = False

self.internet\_latency = 999.0

self.last\_correction = time.time() - 1000 # Start with old corrections

self.correction\_age = 999.0

self.ntrip\_data\_rate = 0.0 # Data rate in kbps

self.ntrip\_data\_rate\_check\_time = time.time()

# Failsafe monitoring

self.monitoring\_thread = None

self.stop\_thread = False

self.active\_failsafe = None

self.in\_recovery = False

self.in\_sleep\_mode = False

self.sleep\_start\_time = 0

self.sleep\_duration = 0

# Statistics for monitoring

self.fix\_drops = [] # List of timestamps when FIX->FLOAT drops occurred

self.position\_history = [] # List of (timestamp, position) tuples

self.drift\_events = [] # List of (timestamp, drift\_size) tuples

# Callbacks

self.on\_failsafe\_triggered = None

self.on\_recovery\_attempt = None

self.on\_rover\_wakeup = None

# Dependencies

self.safety\_module = None

self.in\_failsafe\_mode = False

# Add path tracking fields

self.planned\_path = [] # List of waypoints

self.planned\_heading = 0.0 # Planned heading in degrees

self.current\_heading = 0.0 # Current heading in degrees

self.path\_deviation\_events = [] # List of (timestamp, distance\_dev, heading\_dev) tuples

self.last\_waypoint = None # Last successfully reached waypoint

# Configure simulation parameters for testing

self.simulation\_params = {

"path\_deviation\_prob": 0.01, # Probability of path deviation

"stale\_data\_prob": 0.005, # Probability of stale data per check

"correction\_stale\_prob": 0.005, # Probability of stale corrections

"data\_loss\_prob": 0.005, # Probability of serial data loss

"fix\_drop\_prob": 0.01, # Probability of FIX->FLOAT drop

"drift\_prob": 0.01, # Probability of position drift

"jump\_prob": 0.005, # Probability of position jump

"high\_dop\_prob": 0.01, # Probability of high DOP

"weak\_constellation\_prob": 0.01, # Probability of weak constellation

"multipath\_prob": 0.01, # Probability of signal multipath

"rtk\_loss\_prob": 0.01, # Probability of RTK fix loss

"internet\_latency\_prob": 0.01, # Probability of high internet latency

"internet\_loss\_prob": 0.005, # Probability of complete internet loss

"low\_ntrip\_data\_rate\_prob": 0.005, # Probability of low NTRIP data rate

}

# Updated thresholds based on requirements

self.thresholds = {

"gps\_stale\_data": 0.3, # 300ms without NMEA fix

"gps\_correction\_stale\_age": 0.3, # 300ms correction age

"gps\_correction\_stale\_duration": 2.0, # 5000ms duration

"gps\_data\_loss": 0.3, # 300ms without NMEA on COM port

"fix\_instability\_count": 3, # 3 FIX->FLOAT drops

"fix\_instability\_window": 30.0, # 30000ms window

"persistent\_drift\_count": 6, # 6 drifts

"persistent\_drift\_size": 0.03, # 3cm drift

"persistent\_drift\_window": 20.0, # 20000ms window

"position\_jump\_distance": 0.3, # 30cm jump

"position\_jump\_speed": 0.5, # 0.5m/s implied speed

"high\_dop\_threshold": 3.0, # PDOP > 3.0

"high\_dop\_duration": 5.0, # 5000ms duration

"weak\_constellation\_count": 6, # <6 satellites

"weak\_constellation\_duration": 5.0, # 5000ms duration

"multipath\_drop": 10.0, # 10dB-Hz drop

"multipath\_duration": 5.0, # 5000ms duration

"rtk\_fix\_lost\_duration": 10.0, # 10000ms without RTK-FIX

"ntrip\_latency\_threshold": 1.0, # 1000ms correction age

"ntrip\_latency\_duration": 10.0, # 10000ms duration

"internet\_loss\_corrections": 5.0, # 5000ms without corrections

"internet\_loss\_cellular": 10.0, # 10000ms without cellular

"path\_deviation\_distance": 0.05, # 5cm distance deviation

"path\_deviation\_heading": 5.0, # 5° heading deviation

"low\_ntrip\_data\_rate": 2.4, # 2.4 kbps

"low\_ntrip\_data\_rate\_duration": 30.0, # 30000ms duration

}

# Recovery times based on requirements

self.recovery\_times = {

GPSFailsafeReason.GPS\_STALE\_DATA: 10, # 10s to reconnect GNSS

GPSFailsafeReason.GPS\_CORRECTION\_STALE: 20, # 20s to reconnect NTRIP

GPSFailsafeReason.GPS\_DATA\_LOSS: 15, # 15s to reconnect GNSS

GPSFailsafeReason.GPS\_FIX\_INSTABILITY: 30, # 30s to monitor

GPSFailsafeReason.GPS\_PERSISTENT\_DRIFT: 20, # 20s to monitor

GPSFailsafeReason.GPS\_POSITION\_JUMP: 10, # 10s to stop and check

GPSFailsafeReason.GPS\_HIGH\_DOP: 15, # 15s to wait

GPSFailsafeReason.GPS\_WEAK\_CONSTELLATION: 20, # 20s to wait

GPSFailsafeReason.GPS\_MULTIPATH: 5, # 5s before sleep

GPSFailsafeReason.RTK\_FIX\_LOST: 30, # 30s to monitor

GPSFailsafeReason.INTERNET\_CONNECTION\_SLOW: 20, # 20s to reconnect

GPSFailsafeReason.INTERNET\_CONNECTION\_LOST: 30, # 30s to reconnect

GPSFailsafeReason.MODULE\_COMMUNICATION\_FAILURE: 15, # 15s to reconnect

GPSFailsafeReason.PATH\_DEVIATION: 20, # 20s to adjust path

GPSFailsafeReason.LOW\_NTRIP\_DATA\_RATE: 30, # 30s to reconnect NTRIP

GPSFailsafeReason.UNKNOWN: 10 # 10s default

}

# Sleep duration in seconds (5 minutes)

self.default\_sleep\_duration = 300

logger.info("FailsafeModule initialized in %s mode",

"simulation" if simulation\_mode else "hardware")

def set\_safety\_module(self, safety\_module):

"""Set the safety module reference"""

self.safety\_module = safety\_module

def set\_callbacks(self, on\_failsafe\_triggered: Callable = None,

on\_recovery\_attempt: Callable = None,

on\_rover\_wakeup: Callable = None):

"""Set callback functions"""

self.on\_failsafe\_triggered = on\_failsafe\_triggered

self.on\_recovery\_attempt = on\_recovery\_attempt

self.on\_rover\_wakeup = on\_rover\_wakeup

def connect\_to\_gnss(self) -> bool:

"""

Connect to M2 GNSS receiver through serial port

Returns True if connection successful, False otherwise

"""

if self.simulation\_mode:

logger.info("Running in simulation mode, no physical GNSS connection required")

return True

try:

self.serial\_conn = serial.Serial(self.port, self.baud\_rate, timeout=1)

logger.info(f"Connected to GNSS receiver on {self.port} at {self.baud\_rate} baud")

return True

except Exception as e:

logger.error(f"Failed to connect to GNSS receiver: {e}")

return False

def read\_gnss\_data(self) -> Dict:

"""

Read data from M2 GNSS receiver

Returns a dictionary with parsed GNSS data

"""

if self.simulation\_mode:

# Generate simulated GNSS data

return self.\_generate\_simulated\_gnss\_data()

if not self.serial\_conn or not self.serial\_conn.is\_open:

if not self.connect\_to\_gnss():

return {}

try:

# Read data from serial port

line = self.serial\_conn.readline().decode('ascii', errors='replace').strip()

if not line:

return {}

# Parse NMEA sentence

try:

msg = pynmea2.parse(line)

data = self.\_parse\_nmea\_message(msg)

self.last\_gps\_update = time.time()

return data

except pynmea2.ParseError:

return {}

except Exception as e:

logger.error(f"Error reading GNSS data: {e}")

return {}

def \_parse\_nmea\_message(self, msg) -> Dict:

"""Parse different types of NMEA messages and extract relevant data"""

data = {}

try:

if isinstance(msg, pynmea2.GGA):

# Global Positioning System Fix Data

data["fix\_type"] = int(msg.gps\_qual)

data["satellites"] = int(msg.num\_sats) if msg.num\_sats else 0

data["hdop"] = float(msg.horizontal\_dil) if msg.horizontal\_dil else 99.9

data["position"] = (float(msg.latitude), float(msg.longitude))

data["altitude"] = float(msg.altitude) if msg.altitude else 0.0

data["correction\_age"] = float(msg.age\_gps\_data) if msg.age\_gps\_data else 999.0

# Update fix quality based on GGA quality indicator

if data["fix\_type"] == 4:

data["fix\_quality"] = "FIX" # RTK fixed solution

elif data["fix\_type"] == 5:

data["fix\_quality"] = "FLOAT" # RTK float solution

elif data["fix\_type"] > 0:

data["fix\_quality"] = "GPS" # Standard GPS fix

else:

data["fix\_quality"] = "NONE" # No fix

elif isinstance(msg, pynmea2.GSA):

# GPS DOP and active satellites

data["pdop"] = float(msg.pdop) if msg.pdop else 99.9

data["hdop"] = float(msg.hdop) if msg.hdop else 99.9

data["vdop"] = float(msg.vdop) if msg.vdop else 99.9

data["fix\_type\_3d"] = int(msg.mode\_fix\_type) if msg.mode\_fix\_type else 0

elif isinstance(msg, pynmea2.GSV):

# Satellites in view

if msg.msg\_num == 1: # First message in sequence

self.snr\_values = {} # Reset SNR values

current\_time = time.time()

for sat\_index in range(4): # Each GSV message contains up to 4 satellites

sat\_num\_attr = f"sv\_prn\_{sat\_index + 1}"

snr\_attr = f"snr\_{sat\_index + 1}"

if hasattr(msg, sat\_num\_attr) and hasattr(msg, snr\_attr):

sat\_num = getattr(msg, sat\_num\_attr)

snr = getattr(msg, snr\_attr)

if sat\_num and snr:

if sat\_num not in self.snr\_values:

self.snr\_values[sat\_num] = []

self.snr\_values[sat\_num].append((current\_time, float(snr)))

data["snr\_values"] = self.snr\_values.copy()

elif isinstance(msg, pynmea2.VTG):

# Track made good and ground speed

data["speed"] = float(msg.spd\_over\_grnd\_kmph) / 3.6 # km/h → m/s

data["track"] = float(msg.true\_track) if msg.true\_track else 0.0

elif isinstance(msg, pynmea2.RMC):

# Recommended minimum specific GPS/Transit data

if msg.status == 'A': # A=active, V=void

data["position"] = (float(msg.latitude), float(msg.longitude))

data["speed"] = float(msg.spd\_over\_grnd) \* 0.514444 # knots → m/s

data["track"] = float(msg.true\_course) if msg.true\_course else 0.0

data["timestamp"] = (

msg.datetime.timestamp() if msg.datetime else time.time()

)

except Exception as e:

logger.error(f"Error parsing NMEA message: {e}")

return data

def \_generate\_simulated\_gnss\_data(self) -> Dict:

"""Generate simulated GNSS data for testing"""

current\_time = time.time()

data = {}

# Base values

data["timestamp"] = current\_time

# Simulate realistic values with occasional failures based on simulation parameters

# Add heading information

if hasattr(self, 'current\_heading') and not hasattr(self, 'sim\_heading'):

self.sim\_heading = random.uniform(0, 360)

# Simulate heading

if self.active\_failsafe == GPSFailsafeReason.PATH\_DEVIATION:

# Introduce a significant heading deviation

planned\_heading = getattr(self, 'planned\_heading', 0)

heading\_deviation = random.uniform(6, 20) # More than 5 degrees

if random.random() < 0.5:

data["heading"] = (planned\_heading + heading\_deviation) % 360

else:

data["heading"] = (planned\_heading - heading\_deviation) % 360

else:

# Normal small heading variations

if hasattr(self, 'sim\_heading'):

data["heading"] = (self.sim\_heading + random.uniform(-3, 3)) % 360

self.sim\_heading = data["heading"] # Update for next time

else:

data["heading"] = random.uniform(0, 360)

# Fix type

if self.active\_failsafe == GPSFailsafeReason.RTK\_FIX\_LOST:

data["fix\_quality"] = "FLOAT"

elif self.active\_failsafe == GPSFailsafeReason.GPS\_FIX\_INSTABILITY:

# Occasionally switch between FIX and FLOAT

data["fix\_quality"] = "FLOAT" if random.random() < 0.5 else "FIX"

else:

# Normally provide RTK fix with occasional drops based on probability

if random.random() < self.simulation\_params["fix\_drop\_prob"]:

data["fix\_quality"] = "FLOAT"

else:

data["fix\_quality"] = "FIX"

# Satellites

if self.active\_failsafe == GPSFailsafeReason.GPS\_WEAK\_CONSTELLATION:

data["satellites"] = random.randint(3, 5) # Below threshold of 6

else:

data["satellites"] = random.randint(8, 16) # Normal range

# DOP values

if self.active\_failsafe == GPSFailsafeReason.GPS\_HIGH\_DOP:

data["pdop"] = random.uniform(3.5, 6.0) # Above threshold of 3.0

else:

data["pdop"] = random.uniform(1.2, 2.5) # Normal range

data["hdop"] = data["pdop"] \* random.uniform(0.6, 0.8)

data["vdop"] = data["pdop"] \* random.uniform(0.7, 0.9)

# SNR values

snr\_values = {}

for i in range(1, data["satellites"] + 1):

base\_snr = random.uniform(35, 50) # Normal range

if self.active\_failsafe == GPSFailsafeReason.GPS\_MULTIPATH and random.random() < 0.7:

base\_snr -= random.uniform(12, 20) # Drop by more than 10 dB-Hz

snr\_values[f"G{i}"] = base\_snr

data["snr\_values"] = snr\_values

# Position

if not hasattr(self, 'sim\_position') or not self.sim\_position:

self.sim\_position = (random.uniform(40.0, 41.0), random.uniform(-74.0, -73.0))

# Handle position drift and jumps

if self.active\_failsafe == GPSFailsafeReason.GPS\_POSITION\_JUMP:

# Large jump

jump\_size = random.uniform(0.4, 1.0)

jump\_angle = random.uniform(0, math.pi \* 2)

delta\_lat = jump\_size \* math.cos(jump\_angle) / 111111

delta\_lon = jump\_size \* math.sin(jump\_angle) / (111111 \* math.cos(math.radians(self.sim\_position[0])))

data["position"] = (self.sim\_position[0] + delta\_lat, self.sim\_position[1] + delta\_lon)

elif self.active\_failsafe == GPSFailsafeReason.GPS\_PERSISTENT\_DRIFT:

# Persistent small drifts

drift\_size = random.uniform(0.03, 0.10) # 3-10 cm

drift\_angle = random.uniform(0, math.pi \* 2)

delta\_lat = drift\_size \* math.cos(drift\_angle) / 111111

delta\_lon = drift\_size \* math.sin(drift\_angle) / (111111 \* math.cos(math.radians(self.sim\_position[0])))

data["position"] = (self.sim\_position[0] + delta\_lat, self.sim\_position[1] + delta\_lon)

else:

# Normal small variations

delta\_lat = random.uniform(-0.01, 0.01) / 111111 # ~1cm

delta\_lon = random.uniform(-0.01, 0.01) / (111111 \* math.cos(math.radians(self.sim\_position[0])))

data["position"] = (self.sim\_position[0] + delta\_lat, self.sim\_position[1] + delta\_lon)

self.sim\_position = data["position"] # Update simulated position for next time

# Altitude

data["altitude"] = random.uniform(100.0, 101.0)

# Speed and heading

data["speed"] = random.uniform(0.1, 0.5) # m/s

data["track"] = random.uniform(0, 360) # degrees

# Correction age

if self.active\_failsafe == GPSFailsafeReason.GPS\_CORRECTION\_STALE:

data["correction\_age"] = random.uniform(1.5, 10.0) # Above threshold (1000ms)

elif self.active\_failsafe == GPSFailsafeReason.INTERNET\_CONNECTION\_SLOW:

data["correction\_age"] = random.uniform(1.5, 6.0) # Above threshold (1000ms)

else:

data["correction\_age"] = random.uniform(0.1, 0.8) # Normal range

# NTRIP data rate

if self.active\_failsafe == GPSFailsafeReason.LOW\_NTRIP\_DATA\_RATE:

data["ntrip\_data\_rate"] = random.uniform(0.5, 2.0) # Below threshold (2.4 kbps)

else:

data["ntrip\_data\_rate"] = random.uniform(3.0, 10.0) # Normal range

return data

def update\_path\_info(self, planned\_path: List[Tuple[float, float]] = None,

planned\_heading: float = None,

current\_heading: float = None,

last\_waypoint: Tuple[float, float] = None) -> None:

"""Update the current path planning information"""

if planned\_path is not None:

self.planned\_path = planned\_path

if planned\_heading is not None:

self.planned\_heading = planned\_heading

if current\_heading is not None:

self.current\_heading = current\_heading

if last\_waypoint is not None:

self.last\_waypoint = last\_waypoint

def update\_gps\_status(self, has\_fix: bool = None, fix\_type: str = None,

satellites: int = None, hdop: float = None,

pdop: float = None, position: Tuple[float, float] = None,

altitude: float = None) -> None:

"""Update the current GPS status with new values"""

current\_time = time.time()

# Only update values that are provided

if has\_fix is not None:

self.has\_fix = has\_fix

if fix\_type is not None:

# If changing from FIX to FLOAT, record as a drop event

if self.fix\_type == "FIX" and fix\_type == "FLOAT":

self.fix\_drops.append(current\_time)

# Clean up old drops (more than 30 seconds old)

self.fix\_drops = [t for t in self.fix\_drops if current\_time - t <= self.thresholds["fix\_instability\_window"]]

self.fix\_type = fix\_type

if satellites is not None:

self.satellites = satellites

if hdop is not None:

self.hdop = hdop

if pdop is not None:

self.pdop = pdop

if position is not None:

# Record position for drift/jump detection

self.position\_history.append((current\_time, position))

# Clean up old positions (more than 30 seconds old)

self.position\_history = [(t, p) for t, p in self.position\_history

if current\_time - t <= 30]

# Check for jumps or drifts if we have previous positions

if len(self.position\_history) > 1:

prev\_time, prev\_pos = self.position\_history[-2]

dist = self.\_calculate\_distance(prev\_pos, position)

time\_diff = current\_time - prev\_time

# Only check if time difference is reasonable

if time\_diff > 0:

# Detect jumps (>30cm or implied speed >0.5m/s)

if dist > self.thresholds["position\_jump\_distance"] or (dist / time\_diff) > self.thresholds["position\_jump\_speed"]:

logger.warning(f"Position jump detected: {dist:.2f}m in {time\_diff:.2f}s")

# Detect drifts (>3cm)

if dist > self.thresholds["persistent\_drift\_size"]:

self.drift\_events.append((current\_time, dist))

# Clean up old drift events (more than 20 seconds old)

self.drift\_events = [(t, d) for t, d in self.drift\_events

if current\_time - t <= self.thresholds["persistent\_drift\_window"]]

self.position = position

if altitude is not None:

self.altitude = altitude

self.last\_gps\_update = current\_time

def update\_internet\_status(self, connected: bool = None, latency: float = None) -> None:

"""Update the current internet connection status"""

current\_time = time.time()

if connected is not None:

self.internet\_connected = connected

if latency is not None:

self.internet\_latency = latency

self.last\_internet\_check = current\_time

def update\_correction\_status(self, age: float = None) -> None:

"""Update the current correction status"""

current\_time = time.time()

if age is not None:

self.correction\_age = age

self.last\_correction = current\_time - age

def update\_ntrip\_data\_rate(self, data\_rate: float = None) -> None:

"""Update the current NTRIP data rate in kbps"""

current\_time = time.time()

if data\_rate is not None:

self.ntrip\_data\_rate = data\_rate

self.ntrip\_data\_rate\_check\_time = current\_time

def update\_module\_communication(self) -> None:

"""Update the timestamp for last successful module communication"""

self.last\_module\_comm = time.time()

def \_calculate\_distance(self, pos1: Tuple[float, float], pos2: Tuple[float, float]) -> float:

"""

Calculate the distance between two positions in meters

Uses Haversine formula for accurate earth distance

"""

# For simplicity in simulation, use a flat-earth approximation

# 1 degree latitude = ~111,111 meters

# 1 degree longitude = ~111,111 \* cos(latitude) meters

lat1, lon1 = pos1

lat2, lon2 = pos2

# Convert to radians

lat1\_rad = math.radians(lat1)

lat2\_rad = math.radians(lat2)

lon1\_rad = math.radians(lon1)

lon2\_rad = math.radians(lon2)

# Haversine formula

dlon = lon2\_rad - lon1\_rad

dlat = lat2\_rad - lat1\_rad

a = (math.sin(dlat/2)\*\*2) + math.cos(lat1\_rad) \* math.cos(lat2\_rad) \* (math.sin(dlon/2)\*\*2)

c = 2 \* math.atan2(math.sqrt(a), math.sqrt(1-a))

distance = 6371000 \* c # Earth radius in meters

return distance

def get\_failsafe\_reason(self) -> Optional[GPSFailsafeReason]:

"""

Check all failsafe conditions and return the reason if any is triggered

Returns None if all is well

"""

current\_time = time.time()

# 1. GPS data stale (>300ms without any NMEA fix)

if current\_time - self.last\_gps\_update > self.thresholds["gps\_stale\_data"]:

return GPSFailsafeReason.GPS\_STALE\_DATA

# 2. GPS corrections stale (>1000ms old sustained for >5000ms)

if self.correction\_age > self.thresholds["gps\_correction\_stale\_age"] and current\_time - self.last\_correction > self.thresholds["gps\_correction\_stale\_duration"]:

return GPSFailsafeReason.GPS\_CORRECTION\_STALE

# 3. Serial data loss (>300ms without NMEA on COM port)

if current\_time - self.last\_module\_comm > self.thresholds["gps\_data\_loss"]:

return GPSFailsafeReason.GPS\_DATA\_LOSS

# 4. Fix-status instability (≥3 FIX→FLOAT drops in 30000ms)

if len(self.fix\_drops) >= self.thresholds["fix\_instability\_count"]:

return GPSFailsafeReason.GPS\_FIX\_INSTABILITY

# 5. Persistent drift (≥6 drifts >3cm in 20000ms)

if len(self.drift\_events) >= self.thresholds["persistent\_drift\_count"]:

return GPSFailsafeReason.GPS\_PERSISTENT\_DRIFT

# 6. Position jump (>30cm or implied speed >0.5m/s)

# This is checked during position updates

if len(self.position\_history) >= 2:

last\_time, last\_pos = self.position\_history[-1]

prev\_time, prev\_pos = self.position\_history[-2]

time\_diff = last\_time - prev\_time

if time\_diff > 0:

dist = self.\_calculate\_distance(prev\_pos, last\_pos)

if dist > self.thresholds["position\_jump\_distance"] or (dist / time\_diff) > self.thresholds["position\_jump\_speed"]:

return GPSFailsafeReason.GPS\_POSITION\_JUMP

# 7. High DOP (PDOP >3.0 for >5000ms)

if self.pdop > self.thresholds["high\_dop\_threshold"] and current\_time - self.last\_position\_check > self.thresholds["high\_dop\_duration"]:

return GPSFailsafeReason.GPS\_HIGH\_DOP

# 8. Weak constellation (<6 satellites for >5000ms)

if self.satellites < self.thresholds["weak\_constellation\_count"] and current\_time - self.last\_position\_check > self.thresholds["weak\_constellation\_duration"]:

return GPSFailsafeReason.GPS\_WEAK\_CONSTELLATION

# 9. Signal multipath (C/N₀ drop >10dB-Hz for >5000ms)

# Check for multipath failsafe

for prn in list(self.snr\_values.keys()):

# Clean up entries older than 60 seconds to limit memory usage

self.snr\_values[prn] = [(t, snr) for t, snr in self.snr\_values[prn] if current\_time - t <= 60]

if not self.snr\_values[prn]: # Remove empty lists

del self.snr\_values[prn]

continue

snr\_history = self.snr\_values[prn]

if len(snr\_history) < 2: # Need sufficient history to compare

continue

# Calculate baseline SNR (average over last 30 seconds)

baseline\_snrs = [snr for t, snr in snr\_history if current\_time - t <= 30]

if not baseline\_snrs:

continue

baseline\_avg = sum(baseline\_snrs) / len(baseline\_snrs)

# Get recent SNR values (last 5 seconds)

recent\_snrs = [snr for t, snr in snr\_history if current\_time - t <= self.thresholds["multipath\_duration"]]

# Ensure enough data points (e.g., at least 3) and check if all are below baseline - 10

if len(recent\_snrs) >= 3 and all(snr < baseline\_avg - self.thresholds["multipath\_drop"] for snr in recent\_snrs):

return GPSFailsafeReason.GPS\_MULTIPATH

# 10. RTK fix lost (>10000ms without RTK-FIX)

if self.fix\_type != "FIX" and current\_time - self.last\_position\_check > self.thresholds["rtk\_fix\_lost\_duration"]:

return GPSFailsafeReason.RTK\_FIX\_LOST

# 11. High NTRIP latency (avg correction age >1000ms for >10000ms)

if self.correction\_age > self.thresholds["ntrip\_latency\_threshold"] and current\_time - self.last\_internet\_check > self.thresholds["ntrip\_latency\_duration"]:

return GPSFailsafeReason.INTERNET\_CONNECTION\_SLOW

# 12. Complete internet loss (no corrections >5000ms AND no cell >10000ms)

if not self.internet\_connected and current\_time - self.last\_correction > self.thresholds["internet\_loss\_corrections"] and current\_time - self.last\_internet\_check > self.thresholds["internet\_loss\_cellular"]:

return GPSFailsafeReason.INTERNET\_CONNECTION\_LOST

# 13. Low NTRIP data rate (<2.4 kbps for >30000ms)

if self.ntrip\_data\_rate < self.thresholds["low\_ntrip\_data\_rate"] and current\_time - self.ntrip\_data\_rate\_check\_time > self.thresholds["low\_ntrip\_data\_rate\_duration"]:

return GPSFailsafeReason.LOW\_NTRIP\_DATA\_RATE

# 14. Check for path deviation (if we have a planned path)

if self.planned\_path and len(self.planned\_path) > 0:

deviation\_detected, distance\_dev, heading\_dev = self.check\_path\_deviation(

self.position, self.current\_heading, self.planned\_path, self.planned\_heading)

if deviation\_detected:

# Record this deviation event

self.path\_deviation\_events.append((current\_time, distance\_dev, heading\_dev))

# Clean up old events (more than 15 seconds old)

self.path\_deviation\_events = [(t, d, h) for t, d, h in self.path\_deviation\_events

if current\_time - t <= 15]

# If we have multiple deviation events in a short time, trigger failsafe

if len(self.path\_deviation\_events) >= 3: # At least 3 events

return GPSFailsafeReason.PATH\_DEVIATION

# No failsafe triggered

return None

def start\_monitoring(self) -> None:

"""Start the failsafe monitoring thread"""

if self.monitoring\_thread and self.monitoring\_thread.is\_alive():

logger.warning("Monitoring thread is already running")

return

self.stop\_thread = False

self.monitoring\_thread = threading.Thread(target=self.\_monitoring\_loop, daemon=True)

self.monitoring\_thread.start()

logger.info("Failsafe monitoring started")

def stop\_monitoring(self) -> None:

"""Stop the failsafe monitoring thread"""

self.stop\_thread = True

if self.monitoring\_thread:

self.monitoring\_thread.join(timeout=2)

logger.info("Failsafe monitoring stopped")

def \_monitoring\_loop(self) -> None:

"""Main monitoring loop that runs in a separate thread"""

check\_interval = 0.2 # Check every 200ms

last\_record\_time = time.time()

record\_interval = 5.0 # Record status every 5 seconds

while not self.stop\_thread:

try:

current\_time = time.time()

# Inject simulated failures occasionally in simulation mode

if self.simulation\_mode and not self.active\_failsafe:

self.\_inject\_simulated\_failure()

# Read from actual GNSS receiver if available and not in simulation

if not self.simulation\_mode and (current\_time - self.last\_gps\_update > 1):

gnss\_data = self.read\_gnss\_data()

if gnss\_data:

# Update status based on real data

if "fix\_quality" in gnss\_data:

self.update\_gps\_status(

has\_fix=(gnss\_data["fix\_quality"] != "NONE"),

fix\_type=gnss\_data["fix\_quality"],

satellites=gnss\_data.get("satellites", self.satellites),

hdop=gnss\_data.get("hdop", self.hdop),

pdop=gnss\_data.get("pdop", self.pdop),

position=gnss\_data.get("position", self.position),

altitude=gnss\_data.get("altitude", self.altitude)

)

if "correction\_age" in gnss\_data:

self.update\_correction\_status(age=gnss\_data["correction\_age"])

if "ntrip\_data\_rate" in gnss\_data:

self.update\_ntrip\_data\_rate(data\_rate=gnss\_data["ntrip\_data\_rate"])

self.update\_module\_communication()

# Check for failsafe conditions

if not self.in\_recovery:

reason = self.get\_failsafe\_reason()

if reason:

self.\_handle\_failsafe(reason)

# Log status periodically

if current\_time - last\_record\_time >= record\_interval:

self.\_log\_status()

last\_record\_time = current\_time

# Update last position check time

self.last\_position\_check = current\_time

# Sleep for a bit

time.sleep(check\_interval)

except Exception as e:

logger.error(f"Error in monitoring loop: {e}")

time.sleep(1) # Wait a bit longer on error

def \_inject\_simulated\_failure(self) -> None:

"""Inject a simulated failure for testing purposes"""

# Only run this occasionally

if random.random() > 0.01: # 1% chance per check (5 times per second)

return

# Choose a random failure type weighted by probability

failure\_types = [

(GPSFailsafeReason.GPS\_STALE\_DATA, self.simulation\_params["stale\_data\_prob"]),

(GPSFailsafeReason.GPS\_CORRECTION\_STALE, self.simulation\_params["correction\_stale\_prob"]),

(GPSFailsafeReason.GPS\_DATA\_LOSS, self.simulation\_params["data\_loss\_prob"]),

(GPSFailsafeReason.GPS\_FIX\_INSTABILITY, self.simulation\_params["fix\_drop\_prob"]),

(GPSFailsafeReason.GPS\_PERSISTENT\_DRIFT, self.simulation\_params["drift\_prob"]),

(GPSFailsafeReason.GPS\_POSITION\_JUMP, self.simulation\_params["jump\_prob"]),

(GPSFailsafeReason.GPS\_HIGH\_DOP, self.simulation\_params["high\_dop\_prob"]),

(GPSFailsafeReason.GPS\_WEAK\_CONSTELLATION, self.simulation\_params["weak\_constellation\_prob"]),

(GPSFailsafeReason.GPS\_MULTIPATH, self.simulation\_params["multipath\_prob"]),

(GPSFailsafeReason.RTK\_FIX\_LOST, self.simulation\_params["rtk\_loss\_prob"]),

(GPSFailsafeReason.INTERNET\_CONNECTION\_SLOW, self.simulation\_params["internet\_latency\_prob"]),

(GPSFailsafeReason.INTERNET\_CONNECTION\_LOST, self.simulation\_params["internet\_loss\_prob"]),

(GPSFailsafeReason.PATH\_DEVIATION, self.simulation\_params["path\_deviation\_prob"]),

(GPSFailsafeReason.LOW\_NTRIP\_DATA\_RATE, self.simulation\_params["low\_ntrip\_data\_rate\_prob"]),

]

# Calculate total probability for normalization

total\_prob = sum(prob for \_, prob in failure\_types)

if total\_prob <= 0:

return

# Normalize probabilities

normalized\_probs = [prob/total\_prob for \_, prob in failure\_types]

# Choose a failure type based on probability

chosen\_failure = random.choices(

[failure for failure, \_ in failure\_types],

weights=normalized\_probs,

k=1

)[0]

# Set the active failsafe

# Set the active failsafe

logger.info(f"Injecting simulated failure: {chosen\_failure.value}")

self.active\_failsafe = chosen\_failure

# Make the failure persist for a realistic time

# It will be cleared when recovery is successful

# The \_handle\_failsafe method will be called on the next monitoring cycle

def \_handle\_failsafe(self, reason: GPSFailsafeReason) -> None:

"""Handle a detected failsafe condition"""

if self.active\_failsafe == reason:

# Already handling this failsafe

return

logger.warning(f"GNSS Failsafe triggered: {reason.value}")

self.active\_failsafe = reason

# Call the callback if registered

if self.on\_failsafe\_triggered:

try:

self.on\_failsafe\_triggered(reason)

except Exception as e:

logger.error(f"Error in failsafe callback: {e}")

# Start recovery process

self.start\_recovery()

def start\_recovery(self) -> None:

"""Start the failsafe recovery process"""

if self.in\_recovery:

logger.warning("Already in recovery mode, ignoring new recovery request")

return

self.in\_recovery = True

logger.info(f"Starting recovery for: {self.active\_failsafe.value}")

# Call the recovery callback if registered

if self.on\_recovery\_attempt:

try:

self.on\_recovery\_attempt(self.active\_failsafe)

except Exception as e:

logger.error(f"Error in recovery callback: {e}")

# Start recovery thread

recovery\_thread = threading.Thread(target=self.\_recovery\_process, daemon=True)

recovery\_thread.start()

def \_recovery\_process(self) -> None:

"""

The recovery process runs in a separate thread.

It tries different recovery strategies depending on the failsafe reason.

"""

try:

# Get recovery time for this failure type

recovery\_time = self.recovery\_times.get(self.active\_failsafe, 15)

# Strategy depends on the failure type

if self.active\_failsafe == GPSFailsafeReason.GPS\_STALE\_DATA:

self.\_attempt\_reconnect\_gnss()

elif self.active\_failsafe == GPSFailsafeReason.GPS\_DATA\_LOSS:

self.\_attempt\_reconnect\_gnss()

elif self.active\_failsafe == GPSFailsafeReason.MODULE\_COMMUNICATION\_FAILURE:

self.\_attempt\_reconnect\_gnss()

elif self.active\_failsafe in [GPSFailsafeReason.INTERNET\_CONNECTION\_SLOW,

GPSFailsafeReason.INTERNET\_CONNECTION\_LOST]:

self.\_attempt\_reconnect\_internet()

elif self.active\_failsafe in [GPSFailsafeReason.GPS\_CORRECTION\_STALE,

GPSFailsafeReason.LOW\_NTRIP\_DATA\_RATE]:

self.\_attempt\_reconnect\_ntrip()

elif self.active\_failsafe == GPSFailsafeReason.PATH\_DEVIATION:

self.\_attempt\_path\_recovery()

# Wait for conditions to improve up to recovery\_time seconds

start\_time = time.time()

while time.time() - start\_time < recovery\_time:

# Check if the failsafe condition is still active

current\_reason = self.get\_failsafe\_reason()

if current\_reason is None or current\_reason != self.active\_failsafe:

# Condition is resolved or changed

logger.info(f"Recovery successful for: {self.active\_failsafe.value}")

self.active\_failsafe = None

self.in\_recovery = False

return

# Sleep a bit before checking again

time.sleep(1)

# If we get here, recovery failed within the time limit

logger.error(f"Recovery failed for: {self.active\_failsafe.value}, entering sleep mode")

self.enter\_sleep\_mode()

except Exception as e:

logger.error(f"Error in recovery process: {e}")

self.enter\_sleep\_mode() # Safety measure

finally:

self.in\_recovery = False

def \_attempt\_reconnect\_gnss(self) -> None:

"""Attempt to reconnect to the GNSS receiver"""

logger.info("Attempting to reconnect to GNSS receiver")

if self.simulation\_mode:

# In simulation mode, just wait for the simulated failure to clear

logger.info("Simulation mode: Waiting for GNSS reconnection")

return

# Close existing connection if any

if self.serial\_conn and self.serial\_conn.is\_open:

try:

self.serial\_conn.close()

except Exception as e:

logger.error(f"Error closing serial connection: {e}")

# Try to reconnect

try:

self.serial\_conn = serial.Serial(self.port, self.baud\_rate, timeout=1)

logger.info(f"Reconnected to GNSS receiver on {self.port}")

except Exception as e:

logger.error(f"Failed to reconnect to GNSS receiver: {e}")

def \_attempt\_reconnect\_internet(self) -> None:

"""Attempt to reconnect to the internet"""

logger.info("Attempting to reconnect to internet")

if self.simulation\_mode:

# In simulation mode, just wait for the simulated failure to clear

logger.info("Simulation mode: Waiting for internet reconnection")

return

# In a real implementation, this would attempt to reconnect the cellular modem

# or other internet connection mechanism

def \_attempt\_reconnect\_ntrip(self) -> None:

"""Attempt to reconnect to the NTRIP server"""

logger.info("Attempting to reconnect to NTRIP server")

if self.simulation\_mode:

# In simulation mode, just wait for the simulated failure to clear

logger.info("Simulation mode: Waiting for NTRIP reconnection")

return

# In a real implementation, this would attempt to reconnect to the NTRIP server

def \_attempt\_path\_recovery(self) -> None:

"""Attempt to recover from path deviation"""

logger.info("Attempting to recover from path deviation")

if self.simulation\_mode:

# In simulation mode, just wait for the simulated failure to clear

logger.info("Simulation mode: Adjusting path")

return

# In a real implementation, this would:

# 1. Alert the operator

# 2. Attempt to adjust the path

# 3. If unsuccessful, return to the last waypoint

if self.last\_waypoint:

logger.info(f"Returning to last waypoint: {self.last\_waypoint}")

# Code to navigate back to last waypoint would go here

def enter\_sleep\_mode(self, sleep\_duration: int = None) -> None:

"""

Enter sleep mode for a specified duration (default 5 minutes).

In sleep mode, the rover will stop all operations to prevent dangerous behavior.

"""

if self.in\_sleep\_mode:

logger.warning("Already in sleep mode, ignoring new sleep request")

return

# Use the default sleep duration if none specified

if sleep\_duration is None:

sleep\_duration = self.default\_sleep\_duration

logger.warning(f"Entering sleep mode for {sleep\_duration} seconds")

self.in\_sleep\_mode = True

self.sleep\_start\_time = time.time()

self.sleep\_duration = sleep\_duration

# Signal to safety module if available

if self.safety\_module:

try:

self.safety\_module.emergency\_stop("GNSS Failsafe: " + self.active\_failsafe.value)

except Exception as e:

logger.error(f"Error signaling safety module: {e}")

# Start the sleep thread

sleep\_thread = threading.Thread(target=self.\_sleep\_process, daemon=True)

sleep\_thread.start()

def \_sleep\_process(self) -> None:

"""Process that runs during sleep mode"""

try:

# Sleep for the specified duration

time.sleep(self.sleep\_duration)

# Wake up

self.wake\_up()

except Exception as e:

logger.error(f"Error in sleep process: {e}")

# Try to wake up anyway

self.wake\_up()

def wake\_up(self) -> None:

"""Wake up from sleep mode"""

if not self.in\_sleep\_mode:

logger.warning("Not in sleep mode, ignoring wake up request")

return

logger.info("Waking up from sleep mode")

self.in\_sleep\_mode = False

self.active\_failsafe = None

# Reset all status counters and histories

self.fix\_drops = []

self.position\_history = []

self.drift\_events = []

self.path\_deviation\_events = []

# Signal to safety module if available

if self.safety\_module:

try:

self.safety\_module.clear\_emergency("GNSS Failsafe wake up")

except Exception as e:

logger.error(f"Error signaling safety module: {e}")

# Call the wake up callback if registered

if self.on\_rover\_wakeup:

try:

self.on\_rover\_wakeup()

except Exception as e:

logger.error(f"Error in wake up callback: {e}")

def get\_drift\_severity(self) -> DriftSeverity:

"""

Get the current drift severity level based on drift events

Returns a DriftSeverity enum value

"""

if not self.drift\_events:

return DriftSeverity.NONE

# Calculate average drift size

avg\_drift = sum(d for \_, d in self.drift\_events) / len(self.drift\_events)

# Determine severity based on average drift and number of events

if avg\_drift < 0.05 and len(self.drift\_events) < 3:

return DriftSeverity.LOW

elif avg\_drift < 0.10 and len(self.drift\_events) < 5:

return DriftSeverity.MEDIUM

else:

return DriftSeverity.HIGH

def get\_recommended\_action(self) -> DriftAction:

"""

Get the recommended action based on current GPS status

Returns a DriftAction enum value

"""

# If already in sleep mode, recommend sleep

if self.in\_sleep\_mode:

return DriftAction.SLEEP

# If an active failsafe is being handled, check if recovery is in progress

if self.active\_failsafe:

if self.in\_recovery:

return DriftAction.PAUSE

else:

return DriftAction.STOP

# Otherwise, check drift severity

drift\_severity = self.get\_drift\_severity()

if drift\_severity == DriftSeverity.NONE:

return DriftAction.CONTINUE

elif drift\_severity == DriftSeverity.LOW:

return DriftAction.CONTINUE

elif drift\_severity == DriftSeverity.MEDIUM:

return DriftAction.SLOW\_DOWN

else: # HIGH

return DriftAction.PAUSE

def \_log\_status(self) -> None:

"""Log the current status for monitoring"""

status = {

"timestamp": datetime.now().isoformat(),

"has\_fix": self.has\_fix,

"fix\_type": self.fix\_type,

"satellites": self.satellites,

"pdop": self.pdop,

"hdop": self.hdop,

"position": self.position,

"internet\_connected": self.internet\_connected,

"correction\_age": self.correction\_age,

"ntrip\_data\_rate": self.ntrip\_data\_rate,

"active\_failsafe": self.active\_failsafe.value if self.active\_failsafe else None,

"in\_recovery": self.in\_recovery,

"in\_sleep\_mode": self.in\_sleep\_mode,

"drift\_severity": self.get\_drift\_severity().value,

"recommended\_action": self.get\_recommended\_action().value

}

logger.info(f"GNSS Status: {json.dumps(status, default=str)}")

# In a real implementation, this data might be sent to a monitoring system

def get\_status\_report(self) -> Dict:

"""

Generate a detailed status report for external systems

Returns a dictionary with all relevant status information

"""

current\_time = time.time()

status = {

"timestamp": datetime.now().isoformat(),

"gps": {

"has\_fix": self.has\_fix,

"fix\_type": self.fix\_type,

"satellites": self.satellites,

"pdop": self.pdop,

"hdop": self.hdop,

"vdop": self.vdop,

"position": self.position,

"altitude": self.altitude,

"last\_update": self.last\_gps\_update,

"time\_since\_update": current\_time - self.last\_gps\_update

},

"internet": {

"connected": self.internet\_connected,

"latency": self.internet\_latency,

"last\_check": self.last\_internet\_check,

"time\_since\_check": current\_time - self.last\_internet\_check

},

"corrections": {

"age": self.correction\_age,

"last\_update": self.last\_correction,

"time\_since\_update": current\_time - self.last\_correction,

"ntrip\_data\_rate": self.ntrip\_data\_rate

},

"failsafe": {

"active": self.active\_failsafe.value if self.active\_failsafe else None,

"in\_recovery": self.in\_recovery,

"in\_sleep\_mode": self.in\_sleep\_mode,

"sleep\_start\_time": self.sleep\_start\_time,

"sleep\_duration": self.sleep\_duration,

"time\_in\_sleep": current\_time - self.sleep\_start\_time if self.in\_sleep\_mode else 0

},

"drift": {

"severity": self.get\_drift\_severity().value,

"recommended\_action": self.get\_recommended\_action().value,

"recent\_events": len(self.drift\_events),

"fix\_drops": len(self.fix\_drops)

},

"path": {

"deviation\_events": len(self.path\_deviation\_events),

"has\_planned\_path": len(self.planned\_path) > 0,

"last\_waypoint": self.last\_waypoint

}

}

return status

def check\_path\_deviation(self, current\_position: Tuple[float, float],

current\_heading: float,

planned\_path: List[Tuple[float, float]],

planned\_heading: float) -> Tuple[bool, float, float]:

"""

Check if the rover has deviated from its planned path.

Args:

current\_position: Current (latitude, longitude) position

current\_heading: Current heading in degrees

planned\_path: List of (latitude, longitude) waypoints for the planned path

planned\_heading: Planned heading in degrees

Returns:

Tuple of (deviation\_detected, distance\_deviation, heading\_deviation)

"""

# Find the closest point on the planned path

min\_distance = float('inf')

closest\_index = 0

for i, waypoint in enumerate(planned\_path):

distance = self.\_calculate\_distance(current\_position, waypoint)

if distance < min\_distance:

min\_distance = distance

closest\_index = i

# Calculate the heading of the planned path at this point

if closest\_index < len(planned\_path) - 1:

next\_point = planned\_path[closest\_index + 1]

planned\_segment\_heading = self.\_calculate\_heading(

planned\_path[closest\_index], next\_point)

else:

# Use the provided planned heading if we're at the last waypoint

planned\_segment\_heading = planned\_heading

# Calculate heading deviation (normalize to -180 to 180 degrees)

heading\_diff = current\_heading - planned\_segment\_heading

while heading\_diff > 180:

heading\_diff -= 360

while heading\_diff < -180:

heading\_diff += 360

heading\_deviation = abs(heading\_diff)

# Check against thresholds

distance\_deviation = min\_distance

deviation\_detected = (distance\_deviation > self.thresholds["path\_deviation\_distance"] or # 5 cm threshold

heading\_deviation > self.thresholds["path\_deviation\_heading"]) # 5 degrees threshold

return deviation\_detected, distance\_deviation, heading\_deviation

def \_calculate\_heading(self, point1: Tuple[float, float], point2: Tuple[float, float]) -> float:

"""

Calculate the heading from point1 to point2 in degrees from north.

Args:

point1: Starting position (latitude, longitude)

point2: Ending position (latitude, longitude)

Returns:

Heading in degrees (0-360)

"""

lat1, lon1 = math.radians(point1[0]), math.radians(point1[1])

lat2, lon2 = math.radians(point2[0]), math.radians(point2[1])

# Calculate heading using Great Circle formula

dlon = lon2 - lon1

x = math.sin(dlon) \* math.cos(lat2)

y = math.cos(lat1) \* math.sin(lat2) - math.sin(lat1) \* math.cos(lat2) \* math.cos(dlon)

heading = math.degrees(math.atan2(x, y))

# Normalize to 0-360 degrees

return (heading + 360) % 360

class SimulationExample:

"""

Example usage of the FailsafeModule in simulation mode

"""

def \_\_init\_\_(self):

self.failsafe = FailsafeModule(simulation\_mode=True)

self.failsafe.set\_callbacks(

on\_failsafe\_triggered=self.on\_failsafe,

on\_recovery\_attempt=self.on\_recovery,

on\_rover\_wakeup=self.on\_wakeup

)

def on\_failsafe(self, reason):

print(f"FAILSAFE TRIGGERED: {reason.value}")

def on\_recovery(self, reason):

print(f"RECOVERY STARTED: {reason.value}")

def on\_wakeup(self):

print("ROVER WAKING UP")

def run\_simulation(self, duration=300):

"""Run a simulation for the specified duration in seconds"""

print(f"Starting GNSS failsafe simulation for {duration} seconds")

# Start monitoring

self.failsafe.start\_monitoring()

try:

start\_time = time.time()

while time.time() - start\_time < duration:

# Generate some simulated GNSS data

if not self.failsafe.in\_sleep\_mode:

gnss\_data = self.failsafe.\_generate\_simulated\_gnss\_data()

# Update status based on simulated data

if "fix\_quality" in gnss\_data:

self.failsafe.update\_gps\_status(

has\_fix=(gnss\_data["fix\_quality"] != "NONE"),

fix\_type=gnss\_data["fix\_quality"],

satellites=gnss\_data.get("satellites", self.failsafe.satellites),

hdop=gnss\_data.get("hdop", self.failsafe.hdop),

pdop=gnss\_data.get("pdop", self.failsafe.pdop),

position=gnss\_data.get("position", self.failsafe.position),

altitude=gnss\_data.get("altitude", self.failsafe.altitude)

)

if "correction\_age" in gnss\_data:

self.failsafe.update\_correction\_status(age=gnss\_data["correction\_age"])

if "ntrip\_data\_rate" in gnss\_data:

self.failsafe.update\_ntrip\_data\_rate(data\_rate=gnss\_data["ntrip\_data\_rate"])

# Simulate random internet status

if random.random() < 0.01: # 1% chance to change internet status

self.failsafe.update\_internet\_status(

connected=(random.random() < 0.9), # 90% chance of being connected

latency=random.uniform(50, 200)

)

self.failsafe.update\_module\_communication()

# Print status occasionally

if int(time.time()) % 5 == 0:

status = self.failsafe.get\_status\_report()

action = self.failsafe.get\_recommended\_action()

failsafe\_status = "ACTIVE" if self.failsafe.active\_failsafe else "NORMAL"

print(f"Time: {int(time.time() - start\_time)}s | "

f"Fix: {status['gps']['fix\_type']} | "

f"Sats: {status['gps']['satellites']} | "

f"Status: {failsafe\_status} | "

f"Action: {action.value}")

time.sleep(0.2)

except KeyboardInterrupt:

print("Simulation interrupted")

finally:

# Stop monitoring

self.failsafe.stop\_monitoring()

print("Simulation ended")

if \_\_name\_\_ == "\_\_main\_\_":

"""Run a sample simulation when the module is executed directly"""

sim = SimulationExample()

sim.run\_simulation(duration=120) # Run for 2 minutes

S corrections stale (>1000ms old sustained for >5000ms)", "in\_recovery": true, "in\_sleep\_mode": false, "drift\_severity": 0, "recommended\_action": "Pause movement"}

⬆️ COMMAND: Move forward 1.60m

📍 UTM: [380003.39, 2044899.35] (Zone 45N)

📍 Lat/Lon: [18.491113°N, 85.863359°E]

📍 Heading: 167.8° (Compass Heading: 282.2° West-Northwest)

⚠️ Path deviation: 65.00 cm (exceeds 5 cm RTK fixed tolerance)

=== ROVER STATUS [21:10:27] ===

GPS Fix: GPS

Satellites: 9

HDOP: 2.0

Position (Lat/Lon): 18.569726, 73.816804

Current Position (UTM): 3.390, 19.350

📍 Diagonal movement: dx=-3.3900, dy=0.6500, heading=169.1°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 169.1°

Distance to Waypoint: 3.452m

====================

⚠️ Invalid GPS position data

⚠️ Invalid GPS position data

⚠️ Invalid GPS position data

⬆️ COMMAND: Move forward 1.60m

📍 UTM: [380001.83, 2044899.69] (Zone 45N)

📍 Lat/Lon: [18.491116°N, 85.863344°E]

📍 Heading: 167.8° (Compass Heading: 282.2° West-Northwest)

⚠️ Path deviation: 31.00 cm (exceeds 5 cm RTK fixed tolerance)

📡 NMEA: $GNGGA,154019.10,1834.1835933,N,07349.0081454,E,1,09,2.0,566.531,M,-71.775,M,0.0,\*7F

⚠️ Invalid GPS position data

⚠️ Invalid GPS position data

2025-05-22 21:10:28,676,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:28,680,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:28,685,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:28,696,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:28,696,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:28,704,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

⚠️ Invalid GPS position data

⬆️ COMMAND: Move forward 1.60m

📍 UTM: [380000.27, 2044900.03] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863330°E]

📍 Heading: 167.8° (Compass Heading: 282.2° West-Northwest)

📏 Path deviation: 3.00 cm (within RTK fixed tolerance)

=== ROVER STATUS [21:10:28] ===

GPS Fix: GPS

Satellites: 9

HDOP: 2.0

Position (Lat/Lon): 18.569727, 73.816802

Current Position (UTM): 0.270, 20.030

📍 Diagonal movement: dx=-0.2700, dy=-0.0300, heading=186.3°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 186.3°

Distance to Waypoint: 0.272m

====================

2025-05-22 21:10:28,903,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Invalid GPS position data

🛑 COMMAND: Stop

2025-05-22 21:10:28,916,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:28,945,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:28,945,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

✅ Reached target point (0.270, 20.030)

📍 UTM: [380000.00, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863327°E]

📍 Heading: 167.8° (Compass Heading: 282.2° West-Northwest)

⚠️ Invalid GPS position data

📡 NMEA: $GNGGA,154020.50,1834.1836408,N,07349.0080789,E,1,09,2.0,566.432,M,-71.775,M,0.0,\*77

⚠️ Invalid GPS position data

⚠️ Invalid GPS position data

=== ROVER STATUS [21:10:29] ===

GPS Fix: GPS

Satellites: 9

HDOP: 2.0

Position (Lat/Lon): 18.569727, 73.816801

Current Position (UTM): 0.000, 20.000

📍 Vertical movement detected: dy=0.0000, setting heading to 270°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 270.0°

Distance to Waypoint: 0.000m

====================

⚠️ Invalid GPS position data

2025-05-22 21:10:29,954,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:29,959,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:29,959,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

⚠️ Invalid GPS position data

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:29,959,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:29,959,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:29,959,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

⚠️ Invalid GPS position data

✅ TASK 1 COMPLETE: Successfully reached path start point2025-05-22 21:10:30,163,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Invalid GPS position data

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

Current position: (0.000, 20.000)

🛑 COMMAND: Stop

🚜 TASK 2: Aligning rover to path direction...

2025-05-22 21:10:30,231,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

📍 Horizontal movement detected: dx=10.0000, setting heading to 0°

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 TURN: From 167.8° to 0.0°, Direction: turn\_right, Angle: 167.8°

Resetting GPS correction timer without disconnecting

↪️ COMMAND: Turn right 167.8°

2025-05-22 21:10:30,263,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:30,263,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

2025-05-22 21:10:30,295,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Invalid GPS position data

2025-05-22 21:10:30,468,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:30,513,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

📡 NMEA: $GPGSA,A,,,\*56

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

Aligned rover to heading: 0.0°

✅ TASK 2 COMPLETE: Successfully aligned to path direction

2025-05-22 21:10:30,545,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

🚜 TASK 3: Starting path navigation pattern...

2025-05-22 21:10:30,545,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

🚜 COMMAND: Navigate zigzag path with 63 points

2025-05-22 21:10:30,545,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

🌾 Starting in Row 1

🧭 Current direction: ↓ DOWN

➡️ COMMAND: Move from (0.00, 20.00) to (10.00, 20.00)

📍 Horizontal movement detected: dx=10.0000, setting heading to 0°

🎯 Moving to point: (10.00, 20.00) at 1.5 m/s

Distance to target: 10.00m

📍 Horizontal movement detected: dx=10.0000, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380000.08, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863328°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.9200, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.13, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863328°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.8700, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.18, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863329°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.8200, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.23, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863329°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.7700, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.28, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863330°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

Distance to target: 9.72m

📍 Horizontal movement detected: dx=9.7200, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.33, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863330°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.6700, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.38, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863331°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.6200, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.43, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863331°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.5700, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.48, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863332°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.5200, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.53, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863332°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

Distance to target: 9.47m

📍 Horizontal movement detected: dx=9.4700, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380000.60, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863333°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

2025-05-22 21:10:30,752,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:30,756,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:30,764,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:30,764,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

📍 Horizontal movement detected: dx=9.4000, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.65, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863333°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.3500, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.70, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863334°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.3000, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380000.77, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863334°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.2300, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.82, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863335°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

Distance to target: 9.18m

📍 Horizontal movement detected: dx=9.1800, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380000.87, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863335°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.1300, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380000.95, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863336°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=9.0500, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.00, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863337°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

=== ROVER STATUS [21:10:30] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 1.000, 20.000

📍 Horizontal movement detected: dx=-1.0000, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 1.000m

====================

📍 Horizontal movement detected: dx=9.0000, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.05, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863337°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.9500, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.06m

📍 UTM: [380001.11, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863338°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

Distance to target: 8.89m

📍 Horizontal movement detected: dx=8.8900, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.16, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863338°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.8400, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.21, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863339°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.7900, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.26, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863339°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.7400, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.31, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863340°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.6900, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.36, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863340°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

Distance to target: 8.64m

📍 Horizontal movement detected: dx=8.6400, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.41, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863340°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.5900, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.46, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863341°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.5400, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.51, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863341°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.4900, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.56, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863342°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.4400, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.61, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863342°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

Distance to target: 8.39m

📍 Horizontal movement detected: dx=8.3900, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380001.69, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863343°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.3100, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.74, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863344°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.2600, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380001.81, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863344°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.1900, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380001.89, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863345°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=8.1100, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380001.94, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863345°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

Distance to target: 8.06m

📍 Horizontal movement detected: dx=8.0600, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380002.02, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863346°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=7.9800, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380002.10, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863347°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=7.9000, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380002.15, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863347°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=7.8500, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.08m

📍 UTM: [380002.23, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863348°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

📍 Horizontal movement detected: dx=7.7700, setting heading to 0°

✓ Heading diff 0.0° < 10°, no turn needed

⬆️ COMMAND: Move forward 0.05m

📍 UTM: [380002.28, 2044900.00] (Zone 45N)

📍 Lat/Lon: [18.491119°N, 85.863349°E]

📍 Heading: 0.0° (Compass Heading: 90.0° East)

⚠️ Max attempts reached

⚠️ Failed to reach waypoint 2

⚠️ Failed to navigate path. Simulation halted.

Cleaning up resources...

Read error (1/10): 'NoneType' object has no attribute 'hEvent'

✅ Closed global serial connection

Stopping GPS reader...

🛑 Stopping GPS reading...

2025-05-22 21:10:31,766,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:31,767,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:31,767,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:31,767,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:31,767,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:31,767,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

❌ No serial connection available

=== ROVER STATUS [21:10:31] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:31,973,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:31,973,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:31,976,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:31,976,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

2025-05-22 21:10:32,578,rover\_failsafe,INFO,GNSS Status: {"timestamp": "2025-05-22T21:10:32.578071", "has\_fix": true, "fix\_type": "NONE", "satellites": 10, "pdop": 99.9, "hdop": 1.0, "position": [0.0, 0.0], "internet\_connected": true, "correction\_age": 999.0, "ntrip\_data\_rate": 0.0, "active\_failsafe": "GPS corrections stale (>1000ms old sustained for >5000ms)", "in\_recovery": true, "in\_sleep\_mode": false, "drift\_severity": 0, "recommended\_action": "Pause movement"}

❌ No serial connection available

=== ROVER STATUS [21:10:32] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:32,978,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:32,980,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:32,980,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:32,980,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:32,980,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:32,980,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

2025-05-22 21:10:33,183,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:33,183,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:33,185,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:33,193,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

❌ No serial connection available

=== ROVER STATUS [21:10:33] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:34,195,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

📡 Stopped GPS data reading thread

2025-05-22 21:10:34,394,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:34,394,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:34,394,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:34,394,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:34,394,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

--- Logging error ---

Traceback (most recent call last):

File "C:\Users\user\AppData\Local\Programs\Python\Python312\Lib\logging\\_\_init\_\_.py", line 1163, in emit

stream.write(msg + self.terminator)

File "C:\Users\user\AppData\Local\Programs\Python\Python312\Lib\encodings\cp1252.py", line 19, in encode

return codecs.charmap\_encode(input,self.errors,encoding\_table)[0]

^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

UnicodeEncodeError: 'charmap' codec can't encode character '\u2265' in position 91: character maps to <undefined>

Call stack:

File "C:\Users\user\AppData\Local\Programs\Python\Python312\Lib\threading.py", line 1030, in \_bootstrap

self.\_bootstrap\_inner()

File "C:\Users\user\AppData\Local\Programs\Python\Python312\Lib\threading.py", line 1073, in \_bootstrap\_inner

self.run()

File "C:\Users\user\AppData\Local\Programs\Python\Python312\Lib\threading.py", line 1010, in run

self.\_target(\*self.\_args, \*\*self.\_kwargs)

File "F:\GPS\task\_2\_waypoints\sleep\_mode.py", line 752, in \_monitoring\_loop

self.\_inject\_simulated\_failure()

File "F:\GPS\task\_2\_waypoints\sleep\_mode.py", line 840, in \_inject\_simulated\_failure

logger.info(f"Injecting simulated failure: {chosen\_failure.value}")

Message: 'Injecting simulated failure: Persistent drift (≥6 drifts >3cm in 20000ms)'

Arguments: ()

2025-05-22 21:10:34,597,rover\_failsafe,INFO,Injecting simulated failure: Persistent drift (≥6 drifts >3cm in 20000ms)

2025-05-22 21:10:34,714,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:34,714,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:34,722,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:34,722,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:34,722,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

❌ No serial connection available

=== ROVER STATUS [21:10:34] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:34,925,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:34,958,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:35,030,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:35,030,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

2025-05-22 21:10:35,031,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:35,231,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:35,231,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:35,239,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:35,239,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:35,239,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

🔌 Disconnecting from GPS...

2025-05-22 21:10:35,444,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:35,444,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:35,444,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:35,444,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

❌ No serial connection available

=== ROVER STATUS [21:10:35] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:36,448,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:36,649,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:36,651,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:36,651,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:36,660,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:36,660,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

❌ No serial connection available

2025-05-22 21:10:36,860,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:36,860,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:36,860,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:36,860,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

=== ROVER STATUS [21:10:36] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:37,665,rover\_failsafe,INFO,GNSS Status: {"timestamp": "2025-05-22T21:10:37.665177", "has\_fix": true, "fix\_type": "NONE", "satellites": 10, "pdop": 99.9, "hdop": 1.0, "position": [0.0, 0.0], "internet\_connected": true, "correction\_age": 999.0, "ntrip\_data\_rate": 0.0, "active\_failsafe": "GPS corrections stale (>1000ms old sustained for >5000ms)", "in\_recovery": true, "in\_sleep\_mode": false, "drift\_severity": 0, "recommended\_action": "Pause movement"}

❌ No serial connection available

🔌 Disconnect complete

2025-05-22 21:10:37,864,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:37,870,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:37,870,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:37,870,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:37,875,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:37,875,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

=== ROVER STATUS [21:10:37] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:38,075,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:38,075,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:38,081,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:38,081,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

❌ No serial connection available

✅ GPS disconnected successfully

🧹 Cleaning up all GPS connections...

🛑 Stopping GPS reading...

=== ROVER STATUS [21:10:38] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:39,088,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:39,284,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:39,284,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:39,284,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:39,291,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:39,291,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

2025-05-22 21:10:39,492,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:39,493,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:39,494,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:39,497,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

❌ No serial connection available

=== ROVER STATUS [21:10:39] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:40,498,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:40,701,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:40,701,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:40,701,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:40,701,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:40,701,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

❌ No serial connection available

2025-05-22 21:10:40,907,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:40,907,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:40,907,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:40,911,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

=== ROVER STATUS [21:10:40] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

❌ No serial connection available

📡 Stopped GPS data reading thread

🔌 Disconnecting from GPS...

2025-05-22 21:10:41,918,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

=== ROVER STATUS [21:10:41] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:42,115,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:42,115,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:42,115,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:42,121,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:42,121,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

2025-05-22 21:10:42,321,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:42,321,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:42,323,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:42,323,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

2025-05-22 21:10:42,727,rover\_failsafe,INFO,GNSS Status: {"timestamp": "2025-05-22T21:10:42.727092", "has\_fix": true, "fix\_type": "NONE", "satellites": 10, "pdop": 99.9, "hdop": 1.0, "position": [0.0, 0.0], "internet\_connected": true, "correction\_age": 999.0, "ntrip\_data\_rate": 0.0, "active\_failsafe": "GPS corrections stale (>1000ms old sustained for >5000ms)", "in\_recovery": true, "in\_sleep\_mode": false, "drift\_severity": 0, "recommended\_action": "Pause movement"}

❌ No serial connection available

=== ROVER STATUS [21:10:42] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:43,333,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:43,359,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:43,359,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:43,359,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:43,359,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:43,365,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

2025-05-22 21:10:43,564,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:43,564,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:43,567,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:43,567,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

❌ No serial connection available

=== ROVER STATUS [21:10:43] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

🔌 Disconnect complete

2025-05-22 21:10:44,570,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

2025-05-22 21:10:44,572,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:44,574,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:44,582,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

2025-05-22 21:10:44,582,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

2025-05-22 21:10:44,582,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

2025-05-22 21:10:44,785,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:44,785,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:44,785,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:44,791,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

❌ No serial connection available

=== ROVER STATUS [21:10:44] ===

GPS Fix: GPS

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:45,798,rover\_failsafe,INFO,Recovery successful for: GPS corrections stale (>1000ms old sustained for >5000ms)

❌ No serial connection available

2025-05-22 21:10:45,997,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS data stale (>300ms without NMEA fix)

⚠️ Failsafe triggered: GPS data stale (>300ms without NMEA fix)

🛑 COMMAND: Stop

2025-05-22 21:10:45,997,rover\_failsafe,INFO,Starting recovery for: GPS data stale (>300ms without NMEA fix)

🔄 Attempting recovery from GPS data stale (>300ms without NMEA fix)

Resetting GPS data timer without disconnecting

2025-05-22 21:10:45,999,rover\_failsafe,INFO,Attempting to reconnect to GNSS receiver

=== ROVER STATUS [21:10:46] ===2025-05-22 21:10:46,000,rover\_failsafe,INFO,Simulation mode: Waiting for GNSS reconnection

GPS Fix: GPS

2025-05-22 21:10:46,000,rover\_failsafe,INFO,Recovery successful for: GPS data stale (>300ms without NMEA fix)

Satellites: 7

HDOP: 5.4

Position (Lat/Lon): 18.569729, 73.816801

Current Position (UTM): 2.280, 20.000

📍 Horizontal movement detected: dx=-2.2800, setting heading to 180°

Next Waypoint: 0.000, 20.000

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

Heading to Waypoint: 180.0°

Distance to Waypoint: 2.280m

Distance to Waypoint: 2.280m

====================

2025-05-22 21:10:46,201,rover\_failsafe,WARNING,GNSS Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

⚠️ Failsafe triggered: GPS corrections stale (>1000ms old sustained for >5000ms)

🛑 COMMAND: Stop

2025-05-22 21:10:46,201,rover\_failsafe,INFO,Starting recovery for: GPS corrections stale (>1000ms old sustained for >5000ms)

🔄 Attempting recovery from GPS corrections stale (>1000ms old sustained for >5000ms)

Resetting GPS correction timer without disconnecting

2025-05-22 21:10:46,201,rover\_failsafe,INFO,Attempting to reconnect to NTRIP server

2025-05-22 21:10:46,209,rover\_failsafe,INFO,Simulation mode: Waiting for NTRIP reconnection

✅ GPS cleanup complete

Stopping GPS logger...

📡 Stopping GPS data logger

Stopping failsafe monitoring...

2025-05-22 21:10:46,609,rover\_failsafe,INFO,Failsafe monitoring stopped

✅ Cleanup complete